






2nd Jan.2023 
CONFIDENTIAL – NOT TO BE USED BY ANYONE OTHER THAN AUTHORIZED MEMBERS OF LODHA GROUP.

TECHNICAL SPECIFICATIONS – RESIDENCES
	No.
	Subject
	Details

	1
	Name of Project
	LODHA BELLAVISTA

	2
	Name of Building
	LODHA BELLAVISTA

	
3
	Wings (to which these specifications are applicable)
	Specifications are applicable for all types given below:
All flats


	4
	Levels
	1. Drop off level – Ground Floor
2. Upper Levels: STILT+35 
3. Refuge Levels : 8TH,13TH,18TH,23TH,28TH,33TH
4. Total:  BASEMENT 1 & 2, GROUND, PODIUM 1 TO 3, STILT, 35 RESIDENTIAL LEVELS

	
5
	Structural Details
	5. Type of Construction: RCC beam Slab construction.
6. Slab Thickness:

a. Thickness of structural slab –  Residential levels:  125 – 175 mm

b. Thickness of slab at the column capital – NA.
7. Structural Loading Capacity: 

Dead load:

· Concrete = 2500 kg/cu.m.

· Partition wall = 700 kg/cu. m.

· Floor finishes = 100 kg/sq.m.

     Live load:

· Car Park areas = 250 kg/sq.m.

                                                                 -     Toilet area = 200 kg/sq.m.
· All rooms & kitchens = 200 kg/sq.m.

· Staircase, passages & balconies = 300 kq/sqm..

8. Earthquake-resistant structural design as per Seismic Zone III requirements.

	6
	Heights
	Floor to Floor heights (unfinished):

9. B1 ,B2- 2.85M, GROUND-3M, P1 TO P3-2.8M, STILT-3.65M, RESIDENTIAL FLOORS-3.05M
10. Residential Levels: 3.05 m (10’)
11. Total up to terrace level: 122.4 mt. (max.)

	7
	Types and Saleable Area of Residences
	Refer Annexure I

	8
	Loading
	12. As % of carpet area: 65 %

13. As % of saleable area: 39.39%


	9
	Facilities
	14. Clubhouse: AMENITIES A STILT
a. Gymnasium

b. Indoor games area with Table tennis, pool table, carom and chess etc

c. Library  Lounge (In existing development & Exclusive to Bellavista both)
d. Party hall
e. Indoors Kids play area / Crèche (In existing development & Exclusive to Bellavista both)
f. Guest rooms (In existing development)
g. Changing rooms (In existing development)
15. Retail 

16. EV charging point for electric vehicles *

a. Swimming Pool (In existing development)
17. Outdoors kid’s play area

18. Party lawn
Social and meeting spaces
Reading area (In existing development & Exclusive to Bellavista both)
19. Senior Citizen corner

20. Reflexology Path (In existing development
21. Pet walk: Y



	10
	Main Entrance Lobby
	22. Size: 77 sq. mt.
23. Floor-to-Floor Height: 5.8 m
24. Finishing Materials: 

a. Flooring: Marble flooring
b. Dado / Walls: Gypsum Plaster and Paint/imported marble/wooden panel/fabric – as per design
c. Ceiling: POP False Ceiling/wooden or aluminum fins etc. – as per design
d. Whether Air-conditioned: Yes


	11
	Lift Lobby (on all residential floors)
	25. Size: approx. 85 sq. mt. (approx.)
26. Floor-to-Floor Height: 3.05 m (10’)
27. Finishing Materials: 

a. Flooring:  designer tiles
b. Dado / Walls: Gypsum Plaster/Vitrified designer tiles and paint
c. Ceiling: POP False Ceiling

28. Whether Air-conditioned: No

	12
	Parking – provided per unit
	29. Total parking: 600 approx. (provided in Podiums & Basements)
30. 2 Basements & 3 Podiums


	13
	Key Architectural Features / Highlights
	31. Facade

a. Sliding windows above 1.2 m and below fixed Glass

b. RCC with primer and paint

c. Screen for Utility area 

32. Building and Common Areas

a. Themed central landscape area free of vehicular traffic.

b. Separate drop-off for each building.

c. Designer air conditioned Entrance Lobby.
d. Designed floor Lobby
e. CCTV monitoring for Key common areas.
f. Video door phones.
g. Swipe card access to Ground floor lobby
33. Inside Residence

a. Full ht. windows attached to Living room and bedroom.
b. Fully air conditioned homes (except for kitchen, bathrooms, service areas , decks and staff room)

c. Separate Utility area 
d. Gas detectors in Kitchen

e. Emergency alarm in each unit

f. Finished toilets with C.P. Sanitary fittings.



	14
	Finishes / Amenities inside Residence
	34. Details of materials used in Apartment 
Room

Flooring

Wall Finish

Dado (if applicable)

Ceiling

Electric Points


Living / Dining

Marble 
Gypsum plaster and Paint 
Same marble Skirting
Paint

Light - 
Fan –
AC –
Plug - 

Sundeck in Living room
Designer Vitrified Tiles

Paint
Same tile Skirting
Paint
Light –

Study room 
Designer Vitrified Tiles

Gypsum plaster and Paint

Same tile Skirting
Paint
Light –
Fan –
AC –
Plug –

Kitchen

Designer Vitrified Tiles

Gypsum plaster and Paint 

 tiles

Paint

Light - 

Plug – 

Gas leakage detector – 

Exhaust – 

Aqua guard point - 

Master Bedroom

Marbital Vitrified Tile
Gypsum plaster and Paint 

Same tile Skirting

Paint

Light –
Fan –
AC –
Plug – 

Other Bedroom(s)

Marbital Vitrified Tile
Gypsum plaster and Paint 

Same tile Skirting

Paint

Light –
Fan –
AC –
Plug – 

Passage

Marble

Gypsum plaster and Paint 

Same marble Skirting

Paint

Light – 

Master Bedroom Toilet

Designer Vitrified Tile
Designer Vitrified Tile
Designer Vitrified Tile
False ceiling with paint

Light – 
Plug –

Geyser – 

Exhaust - 

Other bed room toilet 

Designer

Vitrified Tile
Designer Vitrified Tile
Designer Vitrified Tile
False ceiling with paint

Light – 
Plug – 

Geyser – 

Exhaust - 

Utility

Ceramic Tiles 

Paint

Same tile Skirting

Paint

Plug –

Floor lobby

designer tile as per design

Gypsum plaster and Paint

Skirting as per design
False ceiling with paint

35. Manufacturer of Electrical switches / sockets: Anchor /or equivalent.
36. Air-conditioning provided: Y
a. Type: Split units
b. Manufacturer: Hitachi/LG or equivalent
c. Location and Tonnage:  as per requirement
37. Kitchen: Kitchen fitted with platform
a. Platform material: Granite
b. Sink manufacturer: Nirali/Future or equivalent

c. Appliances Provided:

i. Chimney: Y/ N                      If Y, Manufacturer: _______________

ii. Stove: Y/ N                            If Y, Manufacturer: _______________

iii. Microwave: Y/ N.                 If Y, Manufacturer: _______________

iv. Dish washer: Y/ N.              If Y, Manufacturer: _______________

v. Washing machine: Y/ N.      If Y, Manufacturer: _______________

38. Toilet Fittings: Details of Manufacturers / Brands:

Room

Shower

WC

WC Fittings

Wash
basin

Basin Fittings

Master Bedroom Toilet-2 BHK

Isenberg/

Grohe or equivalent
Kohler/
 Duravit or equivalent
Isenberg/
Grohe or equivalent
Kohler/
Duravit or equivalent 
Isenberg/

Grohe or equivalent
Other Toilet(s)

Isenberg/

Grohe or equivalent
Kohler/
 Duravit or equivalent
Isenberg/

Grohe or equivalent
Kohler/
Duravit or equivalent 
Isenberg/

Grohe or equivalent
Utility
Hindware/
Parryware or equivalent
Parryware/ jaguar or equivalent
39. Doors
a. Main Door

i. Material: Laminate 
ii. Door Fittings Manufacturer: Ozone/ Pag/ Yale or equivalent.
iii. Door Lock Manufacturer: Ozone/ Pag/ Yale or equivalent.
b. Toilet Doors

i. Material: Laminate finish
ii. Door Fittings Manufacturer: Ozone/ Pag or equivalent.
iii. Door Lock Manufacturer: Ozone/ Pag or equivalent.
c. Other Doors

i. Material: Laminate finish
ii. Door Fittings Manufacturer: Ozone/ Pag or equivalent.
iii. Door Lock Manufacturer: Ozone/ Pag or equivalent 
40. Windows
Room

Type of Window (Sliding / Openable / Fixed / Louvers)

Window Frame Material

Window Glass Specification

Height of window (mtrs.)

Height of window ledge above slab (mtrs.)

Living / Dining

Fixed with Sliding
Powder coated Aluminium

clear glass

Kitchen

Operable or sliding
Powder coated Aluminium
clear glass
Master Bedroom

Fixed with Sliding
Powder coated Aluminium
clear glass
Other Bedroom(s)

Fixed with Sliding
Powder coated Aluminium
clear glass
Master Bedroom Toilet

Openable

Powder coated Aluminium
Frosted glass

Other Toilet(s)

Openable

Powder coated Aluminium
Frosted glass

41. Grills:

a. Whether Provided: N

42. If Y, Material: MS grill or GRC

43. Material used for Railings in living room decks: glass with SS handrail 
44. Material used for Railings in utility and other decks: MS grill or GRC
45. Lofts:

Room

Provided (Y/N)

IF Y, Length; depth (mtrs.)

All rooms
No


	15
	Home Automation
	46. Whether Provided: Not provided

	16
	Security Controls
	47. Complex Entrance: Access Control with boom barrier, RFID access for vehicles

48. Entrance Lobby of Building: swipe card access 

49. Residence: Video Door Phone : Y

50. Inside Residence –Gas detector in Kitchen of residence.
51. Staircase access: Controlled at ground floor and podium top only
52. Parking Area access: RFID cards for vehicles

53. Separate service staff entry: Y(architect to confirm)
54. CCTV Monitoring:

a. Complex Entrance: Yes / No
b. Common Facilities / Areas: Yes / No)

c. Entrance Lobby of Building: Yes / No
d. Lift Lobby (on each floor): Yes / No

55. Other Features:

IBMS Room to monitor the CCTV and Gas Detector alarm/VDP and take immediate action.


	17
	Fire Protection
	56. Fire Sprinklers:

a. Provision of sprinkler riser pipes to serve staircase and lift lobby areas: Y

b. Owner / Building Manager shall provide and maintain duty and standby pumps, with automatic controls, to serve the sprinkler system: Y/ N
c. Water sprinklers shall be provided in all parking areas (basements) : Y/ N
57. Smoke Detectors: Fire alarm system covering lift lobby areas: Y

58. Fire Hydrants / Hose Reels:

a. Fire hydrants / hose reels which shall provide coverage to staircase and lift lobby areas. Y / N
59. Underground and overhead fire fighting tank of appropriate capacity, as per local regulatory requirements. Yes

60. Refuge areas, as per local regulatory requirements. 

 

	18
	Elevators
	61. Passenger Elevators:
a. For each Wing = 2 no. + 2 fire lifts
b. Capacity per Elevator:  
c. Speed:  2.5 m/s

d. Manufacturer: Otis/schindler/Thyssenkrupp or equivalent
e. Other Features:

i. ______________________________________________________

ii. ______________________________________________________
62. Service / Stretcher Elevators: Provided


	19
	Staircases and Landings
	63. No. of risers per floor: 20 
64. Tread Width: 0.25 m 

65. Finishing Materials: 

a. Flooring: cement tiles
b. Dado / Walls: only skirting 
c. Landing Doors: confirming to 2.0 hrs FRD

	20
	Electrical
	66. Cable used from meter room to residence: 

a. Manufacturer: / avocab or equivalent

b. Specifications: FR Flexible wires in recessed conduit.

67. Wires used inside the residence: 

a. Manufacturer: Avocab / / Polycab / Equivalent
                 b.  Specifications: FR copper wires.

68. Lightening arrester provided: YES

	21
	Power (DG) Backup
	69. D.G. Power Backup for the water pumps, fire pumps, elevators and common area emergency lighting of the building shall be provided by the Owners with automatic changeover facility, in case of power failure / shut down.



	22
	Plumbing
	70. Type of Water Supply System: gravity flow system

71. Pipes used for water distribution upto residence:

a. Manufacturer: CPVC Supreme/Astral or equivalent / UPVC supreme / Equivalent
b. Specifications: UPVC pipes Schedule 40/Fittings 80 & cPVC SDR 11

	23
	Water
	72. Potable drinking water connection from local authorities, as per local regulatory norms.

73. Flushing water made available through recycling. 

74. Provision for rain harvesting. Yes

75. Additional water supply source(s):

a. Tanker (Raw water tank is not considered in ACME drgs, Arch to check & confirm)
____________________

	24
	Environment
	76. Recycling of waste water and sewage through Sewage Treatment Plant: Y / N
a. If Y, all sewage generated will be treated through sewage treatment plant at site and recovered water shall be used for flushing and other permissible uses.

77. Provision for rain harvesting : Y 

78. Provision for garbage recycling: Y / N --Yes
79. Provision for Solar Energy for:

a. Common Area Lighting: Y

b. Bathrooms Geysers from Floors  : Y / N 

	25
	Garbage
	80. Segregation of garbage into recyclable (wet) and non-recyclable (dry): YES

81. Garbage Chute provided: Y / N
82. Collection of all non-recyclable garbage by local authorities. :Yes.


	26
	Facilities Management


	83. All facilities, common areas and common equipment in the project shall be maintained by a leading Facilities Management company, referred to as the Building Manager.

84. The Resident / Purchaser shall be liable to pay the Building Manager maintenance charges on monthly basis, as may be fixed by the Building Manager from time to time. These charges shall include charges for:

a. Housekeeping of common areas.

b. Maintenance of common equipment.

c. Security of complex and common areas.

d. Water consumption charges.

85. Bills payable on monthly basis to Building Manager within 15 days of bill, failing which interest @ ___% p.a. will be payable on unpaid amount from date of bill to date of payment.

86. The Building Manager shall also operate the facilities as described under heading ‘Facilities’ and shall charge separate usage, maintenance and memberships charges for the same, as may be fixed from time-to-time.

	27
	Consultants
	87. Master planning: KAPL, India
88. Architectural Design: KAPL, India
89. Structural Design: JW Consultants, India
90. Landscape Design: New Arch LLP, India
91. MEP: PDA, India

	28
	Ground Coverage
	92. Total Plot Area: 5934.9 sq. mt. ( 1.46 acres )

93. Total Landscape and recreational spaces : 4145 sq mt.



Notes:

a. All specified manufacturer names are subject to change with manufacturer of equivalent or better quality, as per discretion of project architect.

b. ‘NA’ – Not Applicable

PAGE  
A

