Project Details

	Sr. No.
	Description
	Details

	1
	Proposal Number 
	

	2
	Name of Project
	Environmental Clearance for Proposed expansion of “Acme Ozone”-Residential cum Commercial Project at Land bearing Gut no 61/1/1, Gut no 61/1/2,3,4, 61/2/1,2,3 at Village Chitalsar - Manpada, Taluka & District Thane by M/s. Acme Housing India Pvt. Ltd. 

	3
	Project category
	8 (b), B1

	4
	Type of Institution
	Private 

	5
	Project Proponent
	Name
	Rupesh kadam

	
	
	Regd. Office address
	

	
	
	Contact number
	9769872565

	
	
	e-mail
	Rupesh.kadam2@lodhagroup.com

	6
	Consultant
	Name: M/s. Enviro Analysts & Engineers Pvt. Ltd.
NABET Accreditation No: NABET/EIA/2023/RA0206
Validity: 13.05.2023

	7
	Applied for
	Brownfield Project 

	8
	Location of the project
	Gut no 61/1/1, Gut no 61/1/2,3,4, 61/2/1,2,3 at Village Chitalsar - Manpada, Taluka & District Thane

	9
	Latitude and Longitude
	KML File with plot boundary marked to be shared	Comment by Rupesh Kadam: Provided 

	10
	Plot Area (Sq.m.)
	54,500 Sq.m

	11
	Deductions (Sq.m.)	Comment by Rupesh Kadam: Liaison
	

	12
	Net Plot area (Sq.m.)	Comment by Rupesh Kadam: Liaison
	

	13
	Ground coverage (m2) & %
	30914 sq.m. ; 57%	Comment by Rupesh Kadam: Design 

	14
	FSI Area (Sq.m.)
	1,92,534.74 Sq.m

	15
	Non-FSI (Sq.m.)
	1,80,926.43 Sq.m

	16
	Proposed built-up area (FSI + Non FSI) (Sq.m.)
	3,73,461.17 Sq.m

	17
	TBUA (m2) approved by Planning Authority till date	Comment by Rupesh Kadam: Liasion
	

	18
	Earlier EC details with Total Construction area, if any.
	SEAC-2014/CR-234/TC-1 dated 28th January 2016

	19
	Construction completed as per earlier EC (FSI + Non FSI) (Sq.m.) 	Comment by Rupesh Kadam: Acme /Design 
	



	[bookmark: _Hlk105068443]20
	Previous EC / Existing Building
	Proposed Configuration	Comment by Rupesh Kadam: Liaison 
	Reason for Modification / Change

	
	Building
Name
	Configuration
	Height
(m)
	Building
Name
	Configuration
	Height
(m)
	

	
	PLOT A
	PLOT A
	

	
	Building no. 1-4 & 8
	Gr.+2P+St.+27 Floors
	91.80
	Building no. 1-4 & 8
	3 lvl Podium (Gr.+2P) + Stilt + FAS + 1st - 26th Floor
	91.80
	No Change

	
	Building no. 5
	Gr. + 2P + Stilt + 27 Floors

	91.80
	Building no. 5
	2 lvl Basement + 4lvl Podium(Gr.+3P)+Stilt+1st- 34th floor

	119.35
	Change in planning

	
	Building no. 6
	Gr. + 2P + Stilt + 27 Floors

	91.80
	Building no. 6
	2 lvl Basement + 4lvl Podium(Gr.+3P)+Stilt+1st- 34th floor

	119.35
	Change in Planning

	
	Building no. 7
	Gr. + 2P + Stilt + 27 Floors

	91.80
	Building no. 7
	1B + Ground(pt)/ 1 level Podium + 1st Floor (pt)/ 2nd Level Podium + 2nd Floor(pt) / 3lvl. Podium (Gr.+2P) + Stilt + FAS + 1st to 26th Floors
	91.80
	Addition of 1 basement

	
	Plot B
	Plot B
	

	
	2 Buildings: Oakwood & Ashwood

	3P + Stilt + 28 Floors

	90.95
	2 Buildings: Oakwood & Ashwood

	3P(Gr.+2P)+St+28 Floors
	90.95
	No Change

	
	MMRDA
	MMRDA
	

	
	Building No.1
	Gr./shops + 25th floor

	76.30
	Building No.1
	Gr./shops + 25th floor

	76.30
	No Change

	
	Building No.2
	Stilt + 25th floor

	76.30
	Building No.2
	Stilt + 25th floor

	76.30
	No Change

	
	Building No.3,4,6
	Gr./shops + 22nd floor

	67.60
	Building No.3,4,6
	Gr./shops + 22nd floor

	67.60
	No Change

	
	Building No.5
	Stilt + 23rd floor

	70.50
	Building No.5
	Stilt + 23rd floor (part)

	70.50
	No Change

	21
	No. of Tenements & Shops
	Plot A: 
Flats: 1369 nos.
Shops: 10 nos.
Offices: 7 nos.

Plot B:
Flats: 382 nos.
Club House: 1 no.

MMRDA:
Flats: 2448 nos.
Shops: 48 nos.
Balwadi: 2 nos.
6 No of Society Office & 5 no of Manager Room
Welfare Centre: 4 nos.

	22
	Total Population
	22183 nos. 

	23
	Total Water Requirements CMD
	2608 KLD

	24
	Under Ground Tank (UGT) location
	Below Ground 

	25
	Source of water
	TMC

	26
	STP Capacity & Technology
	2480 KLD	Comment by Rupesh Kadam: MEP

	27
	STP Location
	

	28
	Sewage Generation CMD & % of sewage discharge in the sewer line  
	2251 
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	Solid Waste Management during Construction Phase
	Type
	Quantity (Kg/d)
	Treatment / disposal

	
	
	Dry waste
	10 kg/day
	Will be handed over to a recycler

	
	
	Wet waste
	25 kg/day
	Handed over to municipal waste collector

	
	
	Construction waste
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	30
	Total Solid Waste Quantities with type during Operation Phase & Capacity of OWC to be installed
	Type
	Quantity (Kg/d)
	Treatment / disposal

	
	
	Dry waste
	6554 kg/day
	Will be handed over to a recycler

	
	
	Wet waste
	4204 kg/day
	Composting by OWC- manure produced will be used at a site for landscaping

	
	
	E-Waste	Comment by Rupesh Kadam: MEP
	
	Will be collected and sent to MPCB authorized recyclers.

	
	
	STP Sludge (dry)	Comment by Rupesh Kadam: MEP
	
	Dry sewage sludge will be used as manure for gardening.

	31
	R.G. Area in sq.m.


		RG required – 3530.66  sq.m ( %)

	RG provided on Mother earth- 3535.2 sq. m. 

	RG provided on the Podium –4540.54 sq.m.

	Total – 8075.74 sq.m 




	
	
	Existing trees on the plot: 

	
	
	Number of trees to be planted: 
a) Along Plot Boundary and R.G. area: 
b) In Miyawaki Plantation: 

	
	
	Number of trees to be cut:  

	
	
	[bookmark: _GoBack]Number of trees to be transplanted: 

	32
	Power requirement



	During Operation Phase:
	Details 
	MSEDCL 

	Connected load (kW)
	42443.3 KW

	Demand load (kW)
	14149.03 KW




	33
	Energy Efficiency
	a) Total Energy saving (%): 
b) Solar energy (%):

	34
	D.G. set capacity
		2 no’s 630 kVA, 1 no. 750 kVA (for E&F tower)

	1 no. 500 kVA

	2 no’s 630 kVA




	35
	No. of 4-W & 2-W Parking with 25% EV 
	4 Wheelers – 2424 Nos, - 
2Wheeler – 2488 nos,.

	36
	No. & capacity of Rain water harvesting tanks /Pits 
	

	37
	Project Cost in (Cr.) 
	952.41

	38
	EMP Cost	Comment by Rupesh Kadam: EMP
	

	39
	CER Details with justification if any….as per MoEF&CC circular dated 01/05/2018
	It will be as per the OM dated 30th September 2020.

	40
	Details of Court Cases/litigations w.r.t the project and project location, if any.
	NA




