Project Details

	Sr. No.
	Description
	Details

	1
	Proposal Number 
	

	2
	Name of Project
	Environmental Clearance for Proposed expansion of “Acme Ozone”-Residential cum Commercial Project at Land bearing Gut no 61/1/1, Gut no 61/1/2,3,4, 61/2/1,2,3 at Village Chitalsar - Manpada, Taluka & District Thane by M/s. Acme Housing India Pvt. Ltd. + Macrotech Developers ltd. 	Comment by Omkar Patil: Application to be made under which Name? Kindly confirm.

	3
	Project category
	8 (b), B1

	4
	Type of Institution
	Private 

	5
	Project Proponent
	Name
	Name of concerned person -Applicant details to be provided

	
	
	Regd. Office address	Comment by Omkar Patil: 	Comment by Omkar Patil: 
	

	
	
	Contact number
	

	
	
	e-mail
	

	6
	Consultant
	Name: M/s. Enviro Analysts & Engineers Pvt. Ltd.
NABET Accreditation No: NABET/EIA/2023/RA0206
Validity: 13.05.2023

	7
	Applied for
	Brownfield Project 

	8
	Location of the project
	Gut no 61/1/1, Gut no 61/1/2,3,4, 61/2/1,2,3 at Village Chitalsar - Manpada, Taluka & District Thane

	9
	Latitude and Longitude
	KML File with plot boundary marked to be shared

	10
	Plot Area (Sq.m.)
	54,500 Sq.m

	11
	Deductions (Sq.m.)
	

	12
	Net Plot area (Sq.m.)
	

	13
	Ground coverage (m2) & %
	30914 sq.m. ; 57%

	14
	FSI Area (Sq.m.)
	1,92,534.74 Sq.m

	15
	Non-FSI (Sq.m.)
	1,80,926.43 Sq.m

	16
	Proposed built-up area (FSI + Non FSI) (Sq.m.)
	3,73,461.17 Sq.m

	17
	TBUA (m2) approved by Planning Authority till date
	

	18
	Earlier EC details with Total Construction area, if any.
	SEAC-2014/CR-234/TC-1 dated 28th January 2016

	19
	Construction completed as per earlier EC (FSI + Non FSI) (Sq.m.) 
	



	[bookmark: _Hlk105068443]20
	Previous EC / Existing Building
	Proposed Configuration
	Reason for Modification / Change

	
	Building
Name
	Configuration
	Height
(m)
	Building
Name
	Configuration
	Height
(m)
	

	
	PLOT A
	PLOT A
	

	
	Building no. 1-4 & 8
	Gr.+2P+St.+27 Floors
	91.80
	Building no. 1-4 & 8
	3 lvl Podium (Gr.+2P) + Stilt + FAS + 1st - 26th Floor
	91.80
	No Change

	
	Building no. 5
	Gr. + 2P + Stilt + 27 Floors

	91.80
	Building no. 5
	2 lvl Basement + 4lvl Podium(Gr.+3P)+Stilt+1st- 34th floor

	119.35
	Change in planning

	
	Building no. 6
	Gr. + 2P + Stilt + 27 Floors

	91.80
	Building no. 6
	2 lvl Basement + 4lvl Podium(Gr.+3P)+Stilt+1st- 34th floor

	119.35
	Change in Planning

	
	Building no. 7
	Gr. + 2P + Stilt + 27 Floors

	91.80
	Building no. 7
	1B + Ground(pt)/ 1 level Podium + 1st Floor (pt)/ 2nd Level Podium + 2nd Floor(pt) / 3lvl. Podium (Gr.+2P) + Stilt + FAS + 1st to 26th Floors
	91.80
	Addition of 1 basement

	
	Plot B
	Plot B
	

	
	2 Buildings: Oakwood & Ashwood

	3P + Stilt + 28 Floors

	90.95
	2 Buildings: Oakwood & Ashwood

	3P(Gr.+2P)+St+28 Floors
	90.95
	No Change

	
	MMRDA
	MMRDA
	

	
	Building No.1
	Gr./shops + 25th floor

	76.30
	Building No.1
	Gr./shops + 25th floor

	76.30
	No Change

	
	Building No.2
	Stilt + 25th floor

	76.30
	Building No.2
	Stilt + 25th floor

	76.30
	No Change

	
	Building No.3,4,6
	Gr./shops + 22nd floor

	67.60
	Building No.3,4,6
	Gr./shops + 22nd floor

	67.60
	No Change

	
	Building No.5
	Stilt + 23rd floor

	70.50
	Building No.5
	Stilt + 23rd floor (part)

	70.50
	No Change

	21
	No. of Tenements & Shops
	Plot A: 
Flats: 1369 nos.
Shops: 10 nos.
Offices: 7 nos.

Plot B:
Flats: 382 nos.
Club House: 1 no.

MMRDA:
Flats: 2448 nos.
Shops: 48 nos.
Balwadi: 2 nos.
6 No of Society Office & 5 no of Manager Room
Welfare Centre: 4 nos.

	22
	Total Population
	22183 nos. 

	23
	Total Water Requirements CMD
	2608 KLD

	24
	Under Ground Tank (UGT) location
	Below Ground 

	25
	Source of water
	TMC

	26
	STP Capacity & Technology
	2480 KLD 2445 KLD MBBR

	27
	STP Location
	

	28
	Sewage Generation CMD & % of sewage discharge in the sewer line  
	2251 
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	Solid Waste Management during Construction Phase
	Type
	Quantity (Kg/d)
	Treatment / disposal

	
	
	Dry waste
	10 kg/day
	Will be handed over to a recycler

	
	
	Wet waste
	25 kg/day
	Handed over to municipal waste collector

	
	
	Construction waste
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	30
	Total Solid Waste Quantities with type during Operation Phase & Capacity of OWC to be installed
	Type
	Quantity (Kg/d)
	Treatment / disposal

	
	
	Dry waste
	6554 kg/day
	Will be handed over to a recycler

	
	
	Wet waste
	4204 kg/day
	Composting by OWC- manure produced will be used at a site for landscaping

	
	
	E-Waste
	
	Will be collected and sent to MPCB authorized recyclers.

	
	
	STP Sludge (dry)
	45 KLD
	Dry sewage sludge will be used as manure for gardening.

	31
	R.G. Area in sq.m.


		RG required – 3530.66  sq.m ( %)

	RG provided on Mother earth- 3535.2 sq. m. 

	RG provided on the Podium –4540.54 sq.m.

	Total – 8075.74 sq.m 




	
	
	Existing trees on the plot: 

	
	
	Number of trees to be planted: 
a) Along Plot Boundary and R.G. area: 
b) In Miyawaki Plantation: 

	
	
	Number of trees to be cut:  

	
	
	Number of trees to be transplanted: 

	32
	Power requirement



	During Operation Phase:
	Details 
	MSEDCL 

	Connected load (kW)
	42443.3 KW

	Demand load (kW)
	14149.03 KW




	33
	Energy Efficiency
	a) Total Energy saving (%): 
b) Solar energy (%):

	34
	D.G. set capacity
		2 no’s 630 kVA, 1 no. 750 kVA (for E&F tower)

	1 no. 500 kVA

	2 no’s 630 kVA




	35
	No. of 4-W & 2-W Parking with 25% EV 
	4 Wheelers – 2424 Nos, - 
2Wheeler – 2488 nos,.

	36
	No. & capacity of Rain water harvesting tanks /Pits 
	

	37
	Project Cost in (Cr.) 
	

	38
	EMP Cost
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	39
	CER Details with justification if any….as per MoEF&CC circular dated 01/05/2018
	It will be as per the OM dated 30th September 2020.

	40
	Details of Court Cases/litigations w.r.t the project and project location, if any.
	NA




