Annexure-01

Scope of works for embedded conduiting for LV and ELV services: 
Following shall be included in vendor scope of works; necessary cost shall be considered by the vendor. 
1. All conduiting shall be done with HMS PVC conduit of size mentioned in the BOQ.
2. Necessary hardware and accessories for conduiting shall be provided by the vendor.
3. All conduiting shall be embedded in slab, RCC wall or floor as required by site conditions. 
4. Vendor shall lay the pull wire or rope through embedded conduits. The pull wire shall be tied with stoppers at both ends so that it will not get pulled back from conduits. Pull wire/rope shall be suitable so as to withstand varied site conditions. 
5. JBs/conduits shall be properly closed with cotton or any other suitable material to avoid its chocking.
6. Vendor shall prepare the shop drawing of conduiting based on the VFC drawings provided for LV/ ELV layouts. Prior to execution vendor shall get approval of these drawings from consultant/client. 
7. Conduit layout shall be prepared by vendor considering shortest possible routes. 
8. Vendor shall prepare and submit the as-built drawings of conduit layout in both soft and hard copies (04 sets each)
9. Chocking of conduits if any shall be rectified by the vendor. Vendor to assist the main contractor with as built drawings, clearing the chocked conduits, pulling of new pull wire/rope (if found missing). 
10. [bookmark: _GoBack]Specs and installation details shall be followed as per tender documents. 
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