TO WHOM SO EVER IT MAY CONCERN

M/s Macrotech Developers Limited (hereinafter referred to as the Company) is developing the “Lodha Acme Ozone” project at Mumbai, Maharashtra. The project is aiming to achieve Platinum certification under the IGBC Green Homes v3 rating System.
The company declares the following:
1. The company declares that the following provisions and amenities will be provided in the project:
a. CO sensors in the covered basement spaces along with axial fans. The CO sensors would modulate the axial fans on the basis of CO levels.
b. In the basements, the air changes per hour (ACH) will be maintained for both normal and fire modes as per the NBC 2016.
2. The company will ensure that the water fixtures used in the project are as per following flow rates -
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*At a design pressure of 4 Bar
3. The company will ensure that rain water harvesting pits and tanks are installed at site as per the credit requirements.
4. The company will ensure that any three of the following irrigation management systems are installed in the project -
a. Central shut-off valve
b. Drip irrigation for the native & adaptive vegetation and sprinklers for the lawn area.
c. Pressure regulating devices to maintain optimal pressure to prevent water loss.
d. Turf and each type of bedding area shall be segregated into independent zones based on watering needs.
5. The company will ensure that the potable water supplied to the project will meet following CPCB specified criteria:
a. Total Coliforms Organism MPN/100ml shall be 5000
b. Less pH between 6 to 9 s
c. Dissolved Oxygen 4mg/l or more
d. Biochemical Oxygen Demand 5 days 20 degrees Celsius 3mg/l or less
6. The company will ensure water meters are installed in the project to monitor the water consumption for following consumption mediums:
a. Landscape water consumption 
b. STP treated water
c. Municipal water consumption
d. Water consumption in club house
e. Flushing water consumption
7. The company will ensure the supply of AC’s for the project is HCFC free, fire suppressions equipment are halon free.

8. The company will ensure following measures are implemented at the design stage:
a. Pumps & Motors: BEE 4-star rated Pumps & Motors of capacity greater than 3 HP and ISI Certified.
b. Efficient Lifts & Escalators with Gearless traction elevators
9. The company will ensure energy meters are installed in the project at the following locations -
a. Common area lighting 
b. Exterior area lighting 
c. Energy meter for lifts 
d. STP energy consumption
e. Domestic Pumps & Motor 
f. Club house 
g. DG set 
h. Solar PV 
i. Firefighting system

10. The company will ensure that the waste water generated will be treated and treated water will be used for landscape and toilet flushing purpose as per the credit requirements.
11. The company will ensure that the atleast 95% of hot water through solar hot water system of hot water requirement and atleast 95% of the annual common area lighting consumption offset through onsite solar PV.
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Water Closets 4/2 LPF
Urinal 1.5 LPF
Lavatory faucets* 4LPM
Kitchen faucets* 4 LPM
Showerheads* 6 LPM
Health Faucet* 6 LPM





