

BUA Calculations:
Total built-up area to be calculated as per p-line.
 For clarity: 
1. Staircases and staircase lobbies, Refuge terraces to be included in built up area. 
2. Lift well to be included in built up area. 
3. Chajjas will not be counted in built-up area. 
4. Elevation features like fins or projections will not be a part of the BUA.
5. The entrance canopies will not be included in the BUA.
6. The shafts/ducts area to be considered only for the slab area & not voids.
7. [bookmark: _GoBack]Terrace, LMR,UGT & OHT areas will not be included in the BUA.


