14.6.13
Approval Rules for Palava 2
27 villages area:
a. MMRDA 27 villages DCR will apply
b. 1 staircase upto 24 m for residential, 2 thereafter.
c. Open space of h/3 and h/5
d. 10% balcony (encloseable) and 10% double height terrace free of FSI
AKB area:
Unit
e. The DCR of A B & C class be will applicable (when sanctioned).
f. Open space of (h/2) – 4 m and h/5. We will try to get limited to 24 m.
g. 15 % balcony (encloseable) and 10 % terraces (double height) are permissible.
h. 1 staircase upto 15 m for residential, 2 thereafter. We will try to get concession upto 24 m but this will remain a moderate risk.
Road width:
	Road Length (as shown in approval from junction)
	Road width

	<= 150 m
	9 m

	150 – 300 m
	12 m

	300 m +
	15 m



Open Space requirements:
a. Dead Side: 6 m
b. L/V side: (h/2 – 4) m, subject to max of 20 m, except front open space
c. Front open space:
a. Road width of 24 m+: 6 m
b. Road width of 15-24 m: 4.5 m
c. Road width <15 m: 3 m
Building height limits (may be possible to drop):
Road width + front open space x 1.5 (however for road width of 18 m+, any height is permissible with front open space of 12 m) (this will be adhered to as much as feasible but compulsorily)
Land allocation:
a. 20% RG (included permissible RG within block)
b. 10% amenities (includes amenities like retail, school, hospital etc if they are standalone; also includes PG)

Based on this, it was agreed as follows:
a. Primary Road: 25 m (distance from block to block)
b. Secondary road between two 19 story blocks: 42 m if possible, else 40 m (distance from block to block)
c. Secondary road between two  8 story blocks: 16 m (distance from block to block)
d. Secondary road between a 8 story block and a 19 story block: 27 m (this ignores the building height requirements)
Additionally,
· Ensure that secondary road length between two junctions does not exceed 300 m.
· Minimize the conditions wherein 8 and 19 storey blocks are facing each other, by using neighbourhood greens, MLCP etc in between.
· We should ensure that each cluster touches a primary road atleast on one side and preferably on two sides.

