01.06.2013
FEEDBACK ON EWS PLANNING, PALAVA
1. 0.2 FSI area to be given for EWS / LIG housing.
2. EWS will have a max BUA area of 27.88 sqm and LIG will have max BUA of 40 sqm.
3. 1RK will be treated as EWS and 1BHK small will be considered as LIG as per Liaison terms.
4. 1 room with shared toilet facilities option not to be considered as will not be acceptable to MMRDA.
5. Units to be designed using maximum BUA permissible in order to reduce number of units.
6. Ratio of both types to be 50% (FSI area) each.
7. Currently designed units to be reviewed again in order to avoid internal ducts, to utilise service ducts to maximum extent and have better efficiency in design.
8. Columns to be designed considering 0.9m balcony projection.
9. Free of FSI wardrobe areas to be avoided.

