24.4.13
MOM – Meeting on 24.4.13
Attendees: KAPL & Lodha
1. Maximize width of the Primary road, to the extent feasible, based on actual width of the building blocks.
2. Minimum footpath width at anytime shall be 2.4 m.
3. Access to cluster green shall be only through the respective building lobbies.
4. Secondary Road:
a. Width: 16 m between outer edge of both buildings (no advantage of cantilever taken)
b. We need 2.4 m footpaths on both sides.
c. Suggested section:
i. Footpath: 2.4 x 2 = 4.8 m
ii. Driveway: 5.5 m
iii. Perpendicular Parking: 4.5 m
iv. Balance: Divided into green buffer
5. Garden apartment: 
a. No ‘garden’ to be provided on the road side facing apartments, save and except those that are between the actual building line and the outer edge of the building (in relation to that apartment).
b. 1.8 m wide garden to be provided in front of the living room / master bedroom for the garden side facing apartments.
6. There shall be one STP per sector. It should be located in the MLCP. In order to facilitate the STP’s functioning, the MLCP should be located at as low a contour as practical (obviously, traffic implications are a larger priority for MLCP location).
7. Currently planned residential block in front of Transport Hub to be converted to Commercial block.
8. Drop offs to be given on two points for each block which are away from junctions.
9. As per Lodha norms:
Each block to be called as “Cluster”
Zone I to be called as “Sector I”
10. Lodha to review feasibility on Gas based water heating system considering no major change in building plans .
11. Lodha to appoint a consultant to design / guide on Town level amenities and also a Gateway design at project entry.
12. Schedule for Sector I:
Infrastructure start – End of June
Bldg Start – October first week
13. Facade:
a. Railings suggested in all bldgs are horizontal, which needs to be vertical considering safety.
b. Corner windows to be reviewed.
c. Entry canopies and balcony / window projections to be reviewed for avoiding misuse of it by residents.
d. Facade windows to be designed considering safety grills.
e. Ground floor plans to be corrected for ramps, privacy of residents.
f. KAPL to review plans for HVAC.
14. Security:
Block level security to be card based access control system.
No manual security to be considered at present.


