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1. Discrepancies in the structural & arch dwgs.
2. Written dimensions over ride actual drafted  structural dwgs.
3. Struc dwgs not to be measured.(not to scale)
4. Slab thk all across the floors will be 150mm thk except for the facade elements in architectural dwgs.
5. S form needs structural dwgs incorporated in the architectural dwgs.
6. The structural dwg to show structural as well as non-structural  elements.
7. Arch. Wall sections to be used for windows and ventilators.
8. Lodha  design to overlap the arch and structural dwgs as a check
9. Base dwg to be arch dwg.
10. Ground floor varying heights- the top part of the form work will be same as that of the upper floors but the lower part will have different set of form work. 
11. The sill hts of the ground floor will vary but the lintel level will be same
12. For lower part will have to be from the same formwork no new form work
13. Drip moulds in the chajjas & the top surface to be sloped.
14. Lodha struct to give an upstand for the staircase terminating down and continue the staircase in convention downwards.
15. Extra steps in the ground floor flight can be equalized in the finishing later.
16. Lower max 450mm shuttering to be in conventional formwork. Since max two repetitions and hence will be a dis advantage for mivan 80 odd repititions.
17.  lintel provisions  any provision kept to be visible & not embedded.
