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	Particulars
	Discussion
	Remarks

	Residential
	For the FSI purpose we should go ahead with maximum G+7 bldgs & the land parcels should be kept reserved for the 90m high bldgs in future.

	

	Residential
	The 90 m high bldgs can be Aspiration or Hi end Casa depending on the management decision at that time. These parcels to be approximately 20% of the net plot area.
	

	Residential
	The open space rules will be as follows for bldgs up to 24m height:
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Live to Live- H/3+H/3
Dead to dead- H/5+H/5
Live to dead - H/3+H/5

For bldgs above 24m height , the long length factor will be applicable plus the open space as per NBC.

Example:

For a cluster length of 100m & bldg height of 27m 
100-40=60m (Long length after every 40m)
10% of 60= 6m
Therefore 6m+9m (as per adjacent NBC table)= 15m
Hence the bldg to bldg clear distance will be 15m



	

	Residential
	For our case we have G+7 bldg which will be 24m in height & hence there will be no long length factor applicable.
Accordingly the open space required as per live to live will be 8+8= 16m.
But to accommodate one more parking & foot path on one side only we will need the ROW to be 17m.
2m Footpath+ 4.5m parking+6m driveway+4.5m Parking


	

	Residential
	To increase the ground coverage the ROW to be kept optimum. Hence the flatter/straight typology is preferred to a T typology.
	Also looking at the sales of LSG the 2.5bhk is a better selling product.

	Residential
	The straight typology core to have the lift core walls shared with Kitchen or a Living room to avoid the lift noise at night in the bedroom area.
	

	School
	For the schools we need to focus on the liveability factor rather than fitting in to the liaison requirement.
Hence concluded that the school nos to be based on population. 
	

	School-Sector 3
	For Sector 3 we have to do 2 schools & the PG to be extended across the road.
	Liaison will have to check the approval fitment of the PG across the road. 

	School-Sector 4
	For Sector 4 we will have to go with 1 School & a Sector club. Since we will not get a 10 acres consolidated land parcel in it.
	1 School & a Sector Club will be bare minimum requirement.

	Visitor Centre
	Visitor centre to be shifted to the Retail depending on the Retail development.
	Sonal

	Admin Office
	Administration office can be in the Retail.
	

	OC
	For the OC requirement we should be doing the following:
1. Fire station.
2. Schools
3. Club Houses
4. EWS

	The fire station can be built for the OC purpose & the Fire engine can be brought from phase 1 at the time of inspection.
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