Palava Phase II – Typology wise Sample Flat for Sector 3
Meeting with Design Team held on 15th Dec 14
1) Flooring & Tiling
a) Living Room – Marbital Floor. Shortlisted for each A & B Type after physical sample review.
b) Kitchen – Vitrified Floor & Dado. Shortlisted but to be checked whether same or diff for A & B type. 
c) Toilets
A Type – 2 combinations of Floor + Wall.
B Type – 2 combinations of floor + Wall. Additional 3rd type is for choice.
d) Wooden Floor – To be checked whether same or diff for A & B type. Actual physical sample awaited from procurement for selection.
e) Utility Floor – Sample shortlisted and awaiting physical sample from procurement.
f) Outside Deck – Sample short listing done and rates awaited from procurement.
g) Staircase – Customized Pavit Tiles option to be checked with procurement since our tread size is 250 mm and available Pavit tiles is usually 300 mm. Pre-cast is the other option but to reduce cost Pavit is being considered.
h) Lift Lobby 
· Wall Dado – Shortlisting to be done. Physical sample to be reviewed.
· Flooring – Shortlisting done after physical sample review.
i) Entrance Lobby 
· Wall Dado – Granite yet to be shortlisted.
· Floor – Tiles shortlisted after physical sample review.
j) Lift Flooring – Yet to be shortlisted.

2) Windows
a) Sample in progress. To be checked with procurement on status.

3) MS Railing – Revised sample to be done as per comments from KAPL discussed as site.  Façade is co-ordinating the same. Sand Blasting & PU Coated panting specified. Costing to be given by Prasad Patil / Ganesh. After costing, value engineering and further design to be issued.

4) Doors

· Laminate for shutters yet to be selected. Main Door Polish + Internal Door Frame Paint colour to be specified by design.

· Hardware – List of Ironmongeries to be specified by design. Make to be provided by procurement.

· Kitchen to Utility Door – Aluminium Door colour and shade selected by design.

· Shaft Doors

a) Internal Flat – Solid / Louvered Metal Doors. Colour Shade & specifications to be selected by design.
b) Lobbies – Same as above.

5) Internal Paint
a) Ceiling – Yet To be selected by design.
b) Walls – Yet To be selected by design.

6) CP / Sanitary Fittings – All shortlisted and sent to procurement. Floor Trap to be checked.

7) Electrical Fittings
· Switch Sockets – Make & Series selected (Legrand, Mylink series).
· Internal DB – Arch. Design requirement is an Integrated DB for both LV and Electrical. Make specified by design is Siemens.

8) Exhausts Fans – Shortlisted but final selection is pending. Physical sample inspected.

9) AC Units – Procurement to advise vendor and make based on technical specifications provided by MEP design. Arch Design to also approve.

10) Geyser – Procurement to advise vendor and make based on technical specifications provided by MEP design. Arch Design to also approve.

11) VDP – Make and Model to be specified by Tushar.



