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plunge. Our 'head - on - shoulders' & 'feet - on - the - ground’
d us to perfect the process and technology, after all it was not rocket science.
than a decade in this business now, we have been able to achieve significant
nsistency in quality, innovation and hard work. These are the three main vital
manufacturing RCC Doorframes with maximum user friendly features and high

date installed more than 05 lakh RCC Doorframe in Pune, Mumbai, Nasik,
um, Karwar and Goa in the last 10 years and we never indulge in calculating
n saved due to this.

Technical Specifications

Concrete Grade of M - 40 with a perfect mix of Cement, Sand,
and Water along with %” and % aggregate

Steel Reinforcement according to the norms laid out in IS - 6523:

For 100 mm X 60 mm Section 03 Bars of 06 mm Round Steel

For 125 mm X 60 mm Section 04 Bars of 06 mm Round Steel
Triangular & Quadrangular Stir ups of 03 mm GI Wire in 100X60
& 125X60 Sections respectively; @ 250 c/c

Specially designed Machinable Poly - Acrylic (MPA) blocks with
ascrew holding capacity of 250 kgs per screw are inserted for fixing
of hinges, night latches, tower bolts, etc.

Water Curing — for 10 days.

Sizes Available (in MM)
Width options: 600 mm to 1800 mm

Height options: 1800 mm to 2400% mm

125 x 60 mm Moulding 125 x 60 mm Double Rebate

Section 5M
R ———

Installing Prowood Ecoframe

100 x 60 mm Moulding

Section 4M

() Each Prowood Ecoframe comes in 03 pieces with 02 vertical members & 01 horizontal member.

Highlights Q®

Table vibrated for maximum compaction
Super smooth finish

Reinforced with round steel bars

100% Foolproof arrangement for fixing of hinges and locks

Very easy to install

>

Saves valuable project time

Arrange it on the floor, as shown in the photograph.

Note: This s ust or the purpose of easing out the weightof the frame.

Made in Reinforced Cement Concrete (RCC) (3 Use the binding wire provided at the ends of every Prowood member to tie the connecting members.





