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                 For Toilet (VF-SX6, but  with gravity shutters)
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                   For Kitchen (VF-AG6)     




          









                                  [image: H:\Palava-Sector 3\Arch\Doc\from vendor\Exhaust fan\pix\IMG_20150310_185356564_HDR.jpg]                                    [image: H:\Palava-Sector 3\Arch\Doc\from vendor\Exhaust fan\pix\IMG_20150310_185403712_HDR.jpg]


            For Ceiling Exhaust fan (VF-BT815)     
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VF-XS Bathroom exhaust fans
(stainless steel panel)

SPECIFICATIONS SPECIFICATIONS
A ‘ : _ Features: . Features:

e Engineering PP plastic body. ® Engineering PP plastic body.

VESRA 220-240 e L 0 100 ® elegantdesign and lower noise. 220240 13 L L 100 #® elegantdesign and lower noise.
VE-X5 220-240 20 120 33 120 TR 220-240

o Silicon steel motor and 100% pure copper winding 'OF ¢ Silicon steel molor and 100% pure copper winding
VF-X6 220-240 25 210 35 150 220-240 i

= ® Built-in thermo-cut-off protect the motor. 6 CF™M ¢ Built-in thermo-cut-off protect the motor.

VF-X8 220-240 25 370 39 200 220-240

® X-8is Eco-motor, condensor motor. : ® XS8is Eco-moior, condensor mofor.

DIMENSION(mm) DIMENSION(mm)

VF-X4 150x140 21 72 98 VF-XS4 150x140 21 72 98
VE-X5 175x163 <] 85 15 VE-XS5 175x163 21 85 115
VF-X6 200x190 25 93 145 VF-XS6 200x190 25 93 145
VF-X8 VF-XS8
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Full Plastic exhaust fans VF-AG Full plastic exhaust fan
(ABS front grille)

SPECIFICATIONS Features: SPECIFICATIONS Features:

o Topgrade PP piastic materiai.Metal body and shutters.
ABS grilie with mat finish.

® elegant design and lower noise

e Topgrade PP p}asﬁc materials.

@ elegant design and lower noise.

VF-AES 220-240 25 330 37 150

¥ VF-AG6 220-240 .

VF-AES 220-240 32 520 40 200 ® Silicon steeimotor and 100% pure copper winding ‘ VF-AGS 220-240 32 530 19 200 @ Silicon steel motor and 100% pure copper winding

: ® Buiiti -cut-off t - ® Built-in thermo-cut- ;
VF-AE10 220-240 42 860 42 250 Buiit-in thermao-cut-off protect the motor VE-AG10 220-240 42 860 42 250 Buiit-in thermo-cut-off protect the motor.
VF-AE{12 % ® Special motor structrue to cause long life and g ® Special molor structrue o cause long life and

220-240 50 1200 47 300 HtAOtor I, | VF-AG12  220-240 50 1200 a7 300 Hobmotor fan
DIMENSION{mm)
DIMENSION(mm)
VF-AES 225x225 30 75 193 : = fezei
VF-AE8 295x300 30 85 242 YEAGE ARAx2%0
VF-AE10 345x350 30 90 290 VE-AG8 290x305 70 85 242
VF-AE12 400x405 30 95 345 VF-AG10 345x350 75 90 290
) VF-AG12 * 400x405 75 95 345

standard i two-way

Static pressure[Pa] Static pressure[Paj
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o VF-BC plastic tubular ceiling ——  VF-BT plastic tubular ceiling exhaust fans

exhaust fan

with ultra cover

SPECIFICATIONS Fanturess SPECIFICATIONS Features:

@ Pilastic body . @ Piastic body

220-240 ‘ 20 150 ; 38 ® clegantdesign and lower noise.

V~BC810 VF-BT&;!!J 220-240 20 150 38 ® czlegantdesign and lower noise.

- S —— TR0 -
VE-BCB15 220-240 24 200 40 . = EBTELS ez Aty ey - , .

@ Silicon steel motor and 100% pure copper winding @ Silicon steel mator and 100% pure copper winding
VE-BC1020 220-240 30 250 43 VF-BT1020 220-240 30 250 43
VF-BC1030 220-240 36 300 45 @ Buiit-in thermo-cui-off protect the moior. i VF-BT1030 220-240 36 300 45 @ Buill-in thermo-cut-off protect the motor.

® Top grade motor ensure fong life ® Top grade motor ensure long fife

@ Fantastic grilie design made from ABS covers : ® Fantastic griile design made from ABS covars

DIMENSIONS(mm) DIMENSIONS(mm)

. R — — VF-BT810  256X256 252
-BC810 25 98 205 25 R
VF-BC8 6X256 20 51 9% 2 caTeis  270Xer0 5

VF-BCB15  270X270 20 51 98 228 265
VF-BT1020  316X316 310

VF-BC1020 316X316 20 51 98 275 310
VF-BC1030 316X316 20 51 98 275 310

VF-BT1030 316X316 10 51 98 275 310
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