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	ELECTRIC WATER HEATER TECHNICAL DATA SHEET
 
	

	 
	 
	SUPERHEAT

	SR.No.
	Heater Volume
	3 Litre instant geyser

	1
	Make
	Superheat ZAP Series

	2
	Model 
	Vertical

	3
	Voltage/Frequency V/Hz
	230V 50Hz AC

	4
	Heater element wattage (Kw)
	3 kw

	5
	Actual standing loss kwh/24h/45⁰C
	Not Applicable

	6
	Max standing loss kwh/24h/45⁰C
	Not Applicable

	7
	Reheating time for 45⁰ C rise in minutes
	2 minutes

	8
	Temperature range ⁰C
	25-75

	9
	Rated water pressure Head in bar
	12

	10
	Inlet & outlet connections in mm
	19

	11
	Overall dimensions(mm)  Dia. X length
	195 × 375

	12
	Thermal cut out provided
	Yes 88 - 96

	13
	Thermostat provided
	Yes

	14
	Pressure relief / Safety cum Non return valve provided
	Yes 110 – 120psi

	15
	CP angle valve provided for inlet
	Optional

	16
	CP angle valve provided for outlet
	Optional

	17
	Outer Tank material
	ABS

	18
	Inner tank meterial
	Jindal SS /304 L

	19
	Inner Tank  protective coating material
	Silicone 

	20
	Type of Body insulation & thickness
	Insul - G

	21
	Heater element material
	Copper

	22
	Heater element protective coating material
	Nickel coated

	23
	Guarantee - overall (Years)
	2 yrs

	24
	Guarantee - Tank (Years)
	10 yrs

	25
	Guarantee - Heater element ( Years)
	4 yrs

	26
	5 Star rating provided
	Not Applicable

	27
	ISI / BS Marked
	IS 8978

	28
	Main cord along with the product 
	Yes provided > 1 mtr

	29
	Water Proof Safety ( IP)
	IP 4

	30
	Compatibility for Celing Hung options for Storage heaters
	No 

	31
	Provision of Brackets / U straps / Channels for Ceiling Suspended Options
	No

	32
	User Friendly LCD/LED indicator
	Green and Red LED Indicator provided

	33
	Anode Material
	NA
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