27.05.2013
Masonary Policy for Palava II
1. External Walls: All external walls to be of 150mm
1. Internal Walls:
1. shared between Staircase and floor lobby-125mm 
1. shared between Flat and Floor lobby-125mm
1. shared between two flats- 125mm
1. all internal walls within a single flat – 100 mm except for:
0. Internal wall adjoining Kitchen Main Counter – 150 mm
0. Internal Toilet walls (including wall adjoining void)-125mm 
0. Internal toilet walls having no fittings / plumbing lines – 100mm
0. Internal Wall adjoining Decks-125mm 
0. Internal Wall housing the DB- 150mm
1. Parapet wall for railing-125 mm


