
CHECK LIST OF ENVIRONMENTAL CLEARANCE 
COMPLIANCE REPORT
To Be Certified by MOEF

Conditions of Environmental Clearance
	Sr.
	Conditions
	Compliance to be confirmed by Project Management
	Complied 
	Photo / Report

	I.
	Construction & Operational phase
	
	
	

	(i)
	All required sanitary and hygienic measures should be in place before starting construction activities and to be maintained throughout the construction phase.
	The sanitation facility is provided separately for gents and ladies.
	YES.
Separate  Urinals and Toilets block are provide strategic location for working staff
	Enclosed

	(ii)
	Provision shall be made for the housing of construction labour within the site with all necessary infrastructure and facilities such as fuel for cooking, mobile toilets, mobile STP, safe drinking water, medical health care, crèche and First Aid Room etc.
	Labour camp is constructed and all necessary facilities are provided to labours like Drinking Water, Sanitary facilities, Kitchen etc.
	YES.
All Infrastructure and Facilities are provided
	Enclosed

	(iii)
	Adequate drinking water and sanitary facilities should be provided for construction workers at the site. Provision should be made for mobile toilets. The safe disposal of wastewater and solid wastes generated during the construction phase should be ensured.
	We have provided drinking water and sanitary facilities to the workers at site.

The biodegradable waste generated from the labour camp is collected in waste bins and this waste is carry out of premise by Third party ensuring further proper disposal.
	YES.
All Infrastructure and Facilities are provided.
	Enclosed

	(iv)
	The solid waste generated should be properly collected and segregated. Dry/inert solid waste should be disposed off to the approved sites for land filling after recovering recyclable material.
	The biodegradable waste generated from the labour camp is collected in waste bins and this is carry out of premise by Third party ensuring further proper disposal.
	YES
	

	(v)
	Wet garbage should be treated by Organic Waste Converter and treated waste (manure) should utilized in the existing premises for gardening. And, no wet garbage will be disposed outside the premises. Local authority should ensure this.
	Project is under construction phase.

 Wet waste which generated from labour camp is dumped into municipal vehicle 

OWC machine for wet waste treatment purpose has been installed at site for completed residential building & IT building.
	YES
	

	(vi)
	Green Belt Development shall be carried out considering CPCB guidelines including selection of plant species and in consultation with the local DFO/Agriculture Dept.
	Green Belt Development will be carried out considering CPCB guidelines
	
	

	(vii)
	The diesel generator sets to be used during construction phase should be low sulphur diesel type and should conform to Environments (Protection) Rules prescribed for air and noise emission standards.

	The DG set which is provided at site is of enclosed type 
	YES
	

	(viii)
	Vehicles hired for the bringing construction material to the site should be good condition and should have a pollution check certificate and should conform to applicable air and noise emission standards and should be operated only during non-peak hours.
	The vehicle hired for bringing construction material to the site is checked for PUC certificate at main gate. 
	YES
	Enclosed

	(x)
	The diesel required for operating DG sets shall be stored in underground tanks and if required, clearance from concern authority shall be taken.
	No diesel has been stored at the site. At the time of requirement, vendor will make availability of the diesel.
	YES
	Enclosed

	(xi)
	Separation of gray & black water should be done by use of dual plumbing line for separation of gray and black water.

	We have provided separate pipe line for gray & black water.
	
	

	(xii)
	Energy conservation measures like installation of CFLs/ TFLs for lighting the area outside the building should be integral part of the project design and should be in place before project commissioning. Use CFLs and TFLs should be properly collected and disposed off/sent for recycling as per the prevailing guidelines/ rule of the regulatory authority to avoid mercury contamination. Use of solar panel may be done to the extent possible like installing solar street lights, common solar water heater system. Project proponent should install, after checking feasibility, Solar plus hybrid non-conventional energy source as source of energy.



	Project is under construction which may issue to maintenance of solar panels 

At operation phase PP will Installed Solar panels for Energy conservation purpose
	
	

	(xiii)
	The installation of Sewage Treatment Plant (STP) should be certified by an independent expert and a report in this regards should be submitted to the MPCB and Environment department before project is commissioned for operation. Discharge of this unused treated affluent, if any should be discharge in the sewer line. Treated effluent emanating from STP shall be recycled/ refused to the maximum extent possible. Discharge of this unused treated affluent, if any should be discharge in the sewer line. Treatment of 100 % gray water by decentralized treatment should be done.  Necessary measures should be made to mitigate the odour problem from STP.

	STP is constructed but not in operation phase
	
	

	(xiv)
	Diesel power generating sets proposed as source of backup power for elevators and common area illumination during operation phase should be of enclosed type and conform to the rules made under the Environmental (Protection) Act, 1986. The height of stack of DG sets should be equal to height needed for the combined capacity of all proposed DG sets. Use low sulphur diesel. The location of the DG sets may be decided with in consultation with Maharashtra Pollution Control Board.
	The DG set which is provided at site is of enclosed type 
	YES
	

	(xv)
	Traffic congestion near the entry and exit points from the roads adjoining the proposed project site must be avoided. Parking should be fully internalized and no public space should be utilized.
	The site is abutting to 60 m wide  road. PP & provided entry and exit gate with security for traffic control at project site. Separate Parking area has been provided within project area.
	YES.
Separate lay by Parking and deployment of Security Personnel to ensure the same.
	Enclosed

	(xvi)
	Regular supervision of the above and other measures for monitoring should be in place all through the construction phase, so as to avoid disturbance to the surroundings.
	Supervisors have been  trained in Environmental Management measures. 
	
	

	(xvii)
	A separate environment management cell with qualified staff shall be set up for implementation of the stipulated environmental safeguards.
	We have management cell  at site with qualified staff for the implementation of the stipulated environmental safeguards.
	
	

	(xviii)
	The Applicant shall draw plans for the segregation of solid wastes into biodegradable and non-biodegradable components. The biodegradable material shall be recycled through scientific in-house composting (i. e. vermi-composting facility within premises) with the approval of local bode. The proper demarcate area shall be identified for collection & storage of MSW properly which, shall be finally disposed off at approved Municipal Solid Waste landfill site of local body environmentally acceptable location and method. I is clarified that the term solid waste includes domestic, commercial and garden wastes, but does not include hazardous and bio-medical waste. The activities of bio-composting and engineered landfill shall be as per the Municipal Solid Waste (M & H) Rules 2000.
	We have provision of segregation of solid waste on site.

Dry garbage has been disposed of to recyclers.

Wet garbage is composted using Mechanical Composting system (Eco Biocompack) and used as organic manure for landscaping
	
	

	(xix)
	Vehicles hired for construction activities should be operated only during non peak hours.
	
	
	

	(xx)
	The applicant, during the construction stage shall provide

a) Septic tank and soak pit of adequate capacity for the domestic effluent generated due to workers residing at site.

b) Proper loading and unloading of construction material, excavated material and its proper disposal as per MSW (M&H) Rules 2000.
	Excavated earth is stacked and re-utilized for backfilling up to plinth.
Excavated Rock and boulders are transported to Crusher (within Premise) for re-utilizing as Granular Sub-Base (GSB) in Road formation works as per IRC.

Construction Debris is utilized in back filling / plot leveling with premise.
	
	

	(xxi)
	The DG set shall be operated only in case of power failure. The applicant shall make arrangement for regular electrical power.
	DG set is only used in case of power failure.
	YES
	

	(xxii)
	Construction equipments generating noise of less than 65/90 dB(A) are permitted.
	Construction equipment generating noise is 69 dB(A) which is within permissible limit 
	YES
	Enclosed

	(xxiii)
	No construction work is permitted during night time.
	We will comply with the condition.
	
	

	(xxiv)
	The Applicant shall take adequate measures for control of noise levels from its own sources within the complex (residential cum Commercial) in respect of noise to less than 55 dB(A) during day time and 45 dB(A) during the night time. Daytime is reckoned as between 6 a.m. to 10 p.m. and Nighttime is reckoned between 10 p.m. to 6 a.m.
	We shall take adequate measures for control of noise levels from sources within the complex
	YES
	Enclosed

	(xxv)
	Solid Waste – The applicant shall provide onsite municipal solid waste processing system & shall comply with Municipal Solid Waste (Management & Handling) Rule 2000 & E-Waste (M & H) Rule 2011
	The biodegradable waste has been treated using OWC and use it as manure.
	
	

	(xxvi)
	In order to ensure that the water from this project do not enter into outside environment, the nallas crossing the township/complex premises, shall be lined, covered and made water tight by the applicant within the premises with intermittent inspection of chambers following good engineering practices as per the regulations of local body.
	We have the provision for the effluent water from construction area i.e should not mixed with water lines of the local area.
	YES
	

	(xxvii)
	Register showing No of Vehicle thro’ & fro’ from site & its PUC details
	
	YES
	Enclosed

	(xxviii)
	Register showing weekly medical check up of site labour
	
	YES
	Enclosed

	(xxix)
	Disposal of sewage from Labour camp thro’ mobile STP or Septic tank & Soak Pit
	Tie up with Third party 

‘3S’ for disposal
	YES
	Enclosed

	(XXX)
	Till date building wise construction work status sheet
	
	
	

	(XXXi)
	Water supply status- Tanker water register
	
	YES
	Enclosed
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