Comparative Statement of Earlier EC & proposed EC proposal. 
Project Casa Bella Dombivali.
	Sr. No.
	Details
	Earlier Proposal whose EC granted dtd.17-07-2010
	Now Proposed

	1
	Name of the Project
	Proposed Construction of Residential Township at villages Nilje,Katai,Usarghar & Ghesar  Taluka Kalyan District – Thane (W). State: Maharashtra.
	Expansion of Residential Township  at villages Nilje, Katai, Usarghar & Ghesar Taluka Kalyan District – Thane (W), State: Maharashtra.

	2
	Project Proponent
	Shri Abhisheck Lodha, M/s.Lodha Dwellers  Pvt. Ltd., Lodha Pavalion, Apollo Mills Compound, N.M.Joshi Marg, Mahalaxmi, Mumbai.
	Shri Abhisheck Lodha, M/s.Lodha Dwellers Pvt. Ltd., Lodha Pavalion, Apollo Mills Compound, N.M.Joshi Marg, Mahalaxmi, Mumbai.

	3
	Location of the Project
	Plot bearing S. No. NILJE - 
	Plot Bearing s. No. NILJE

	4
	Type of Project
	4/1/2/3, 165/1, 166/1A/1B/1C, 166/2, 166/3A/3B, 166/4, 168/0, 169/1 TO 4,5A,5B,6 TO 13, - 170/0,- 171/1 TO 5,- 172/1 TO 4,- 173/1,2, 174/1 TO 3, 175/1 TO 5, 176/1 TO 4, 5A,5B -177/1A,1B,1C,2A,2B-178/0-179/0-180/1,2,- 181/1,2,3, 182/0-183/1A,1B,2,3-184/1P,2,3-185/1A,1B,2 TO 9/10A,10B,11 TO24 -186/1A-1,1A-2,1C,1/4-2 TO 5, 187/0,-188/1,2,-189/1,2-190/1,2,3A,3B, -191/1,2A,2B-192/1A+8A(8A), 1B(1B),1A+8A(8A),1B(1B),1C2(1C2), 191/1C+2A(1C3),192/2B+3A(2B3),2/3(2C),2K+3D(2K4), 3B+7A(3B7), 3C7B(3C7), 4/P(4A), 4P(4C), 5/1(5A1), 5/2 (5A2), 192/6(6)/9(9),193/1,2,3,4A,-201/1A, 1B, 2A1(1C), 2(2),-210/1,2,3A,3B, -214/1,2,-215/0 - 216/1A,1B,1C,1D,2 - 217/0.
	4/2, 4/3,4/7, 4/8A, 105/1,164/1, 164/3, 165/2, 166,166/2, 166/1A, 166/1B, 166/3A, 166/3B, 166/4, 168 pt, 169/1, 169/2, 169/3, 169/4, 169/5A, 169/5B, 169/6, 169/7, 169/8, 169/9, 169/10, 169/11, 169/12, 169/13, 170 pt, 171/1, 171/2, 171/3, 171/4, 171/5, 172/1, 172/2, 172/3, 172/4, 173/1, 173/2, 174/1, 174/2, 174/3, 175/1, 175/2, 175/3, 175/4, 175/5, 176/1, 176/2, 176/3, 176/4, 176/5A, 176/5B, 177/1A, 177/1B, 177/1C, 177/2A, 177/2B, 178 pt, 179pt, 180/1, 180/2, 181/1, 181/2, 181/3, 182 pt, 183/1A, 183/1B, 183/2, 184/1, 184/2, 184/3, 185/1A, 185/1B, 185/2, 185/3, 185/4, 185/5, 185/6, 185/7, 185/8, 185/9, 185/10A, 185/10B, 185/11, 185/12, 185/13, 185/15, 185/16, 185/17, 185/18, 185/19, 185/20, 185/21, 185/22, 185/23, 185/24, 186/1A/1, 186/1A/2, 186/1C, 186/1d, 186/1/4, 186/2, 186/3, 186/4, 186/5, 187, 188/1, 188/2, 189/1, 189/2, 190/1, 190/2, 190/3A, 190/3B, 191/1, 191/2A, 191/2B, 192/1A+8, 192/1B, 192/1+2, 192/1C2, 192/1C3, 192/2B+3A, 192/3B7, 192/2C + 3D, 192/3C7, 192/4A, 192/4C, 192/5A/1, 192/5A/2, 192/6, 192/9, 193/1, 193/2, 193/3, 193/4A, 194/1B, 194/3, 201/1A, 201/1B, 201/2A/1, (201/1C), 201/2, 210,210/2, 210/3A, 210/3B, 214/1, 214/2, 215 pt, 216/1A, 216/1B, 216/1K, 216/1D, 216/2, 217, 165/1, 210/4A, 4/7, 96/1, 96/3, 98/2, 98/3, 98/9, 98/pt, 101/1, 102/5, 102/pt, 103/1, 103/2, 103/3, 104/15, 105/1, 105/2, 106/1, 106/2, 106/3, 106/4, 106/5, 107/1, 107/6A, 107/6B, 107/6C, 108/1A, 108/2, 108/4, 109/3B, 109/4, 109/5B, 123/1, 123/2, 133/4D, 137/2, 138/3, 226/4, 226/5, 232/3, 235/PT, 236/3, 235/2PT, 166/1C, 133/1D, 232/2.

	 
	 
	KATAI -
	KATAI

	 
	 
	7/1A,2A,2B,3A,-8/1A,6A-1,7A,7B,8A,10-A,11C-1,13,14,15, 9/1A,1B,2-10/1,2,-11/1 TO 11,12A,12B,13 TO 22,-12/1,2-13/1,2,-14/0-  15/0,-16/0,-17-0,-18/1,2,3,-19/2 TO 6,-21/4A,83/1,2,-84/1 TO 4,-109/1,2,-122/0
	7/1A, 7/2A, 7/2B, 7/3A, 8/6A/1, 8/7A, 8/7B, 8/8A, 8/10/A, 8/11K/1, 9/1A, 9/1B, 9/2, 10/1, 10/2, 11/1, 11/2, 11/3, 11/4, 11/5, 11/6, 11/7, 11/8, 11/9, 11/10, 11/11, 11/12A, 11/12B, 11/13, 11/14, 11/15, 11/16, 11/17, 11/18, 11/20, 11/21, 11/22, 12/1, 12/2, 13/1, 13/2, 14pt, 15pt,16, 17pt, 18/1, 18/2, 19/3, 19/4, 19/5, 19/6, 21/4A, 83/1, 83/2, 84/1, 84/2, 84/3, 84/4, 109/1, 109/2,122/pt, 134/pt, 8/13, 8/14, 8/15, 11/19, 18/1, 18/3

	 
	 
	USARGAR –
	USARGHAR

	
	
	12/3A,4A,5,6,7,8A,9A,11A,12,13,14A,15A,16,-74/1, 2A, 2B, 2C,3 TO 10, 75/0, 76/1/2A/3A/4A, 5,6,7,8A,8/2,9,10,11-88/0,-89/2A,-105/P,-125/1,2,3A,3B,4,5A,5B,5C,6,7,-137/1, 2,3
	12/3A, 12/4A, 12/5, 12/6, 12/7, 12/8A, 12/9A, 12/11A, 12/12,12/13, 12/14A, 12/15a, 12/16, 74/1, 74/2A, 74/2B, 74/2C, 74/3, 74/4, 74/5, 74/6, 74/7, 74/8, 74/9, 74/10, 75/1, 75/pt,76/1, 76/2a, 76/3a, 76/4a, 76/5, 76/6, 76/7, 76/8A, 76/8B, 76/9, 76/10, 76/11, 88pt, 89/2A, 125/1, 125/2, 125/3A, 125/3B 125/4, 125/5A, 125/5B, 125/5C, 125/6, 125/7, 137/1, 137/2, 137/3, 105pt

	 
	 
	GHESAR – 
	GHESAR

	 
	 
	42, 44/1D, 56/2, 58/P, 58/1B/1, 58/2A, 58/2B, 58/4, 58/6B, 58/7B, 59, 60/1/2/3A/3B/3C, 61/2, 62/1B/2 A/2B/2C/3P/3P /3A/3B/3C/3D/3E/3F/3G/3H/4A/4B/5A/5B, 63/1B1, 63/1B/2 ,63/2, 64/1, 65/1/2, 66/1/2, 66/3A/3B, 66/4, 66/5A/5B, 66/6/7, 67, 68, 74/P, 77/1/2/3/4/5/6, 79, 85/3, 87/1/2/5, 90/1/2/3, 91/1A/1B, 92/1/2, 93, 94/0, 96/1/2, 97/1/2/3/4, 98, 99/1A/1B, 99/2A/2B/2C/2D/2E, 99/3A/3B, 100, 101/ 1A/1B/1C, 101/2, 102/1/2/3, 103, 104/1A, 105/1D, 106/3B, 107/2B/2C, 107/3A/3B/3C, 113/1A, 113/2, 116/P, 116/10, 117, 63/1, 64/2, 69, 70, 71, 72, 73, 74/1, 75, 76, 80, 91/1/1, 95/0, 116/P
	62/3C, 62/3D, 63/1/1,63/1, 64/2, 69, 70, 71, 72, 73, 74/1, 75, 76, 91/1/1, 95, 116/P, 42, 44/1B,44/1C, 44/1D, 53/4B, 56/2, 58/1A2, 58/1B/1, 58/2A, 58/2B, 58/3B, 58/4, 58/5A, 58/5C, 58/6B, 59/-, 60/1, 60/2, 60/3A, 60/3B, 60/3C, 60/3D,61/2, 62Pt 62/1B, 62/2B, 62/2/C, 62/2D, 62/3E, 62/3A, 62/3B,62/3C, 62/3F, 62/3G, 62/3H, 62/4A, 62/4B, 62/5A, 62/5B, 63/1A1, 63/1/4A, 63/1B1, 63/1B/2, 63/2, 62/3B, 64/1, 65/1, 65/2, 66/1, 66/2, 66/3A, 66/3B, 66/4, 66/5A, 66/5B, 66/6, 66/7, 67pt, 68pt, 77/1, 77/2, 77/3, 77/4, 77/5, 77/6, 79/-,80/PT, 81/PT, 87/1, 87/2, 87/5, 103/PT, 90/1, 90/2, 90/3, 91/1A, 91/1B, 91/2, 92/1, 92/2,93pt, 94pt, 96/1, 96/2, 97/3, 97/2, 97/1, 97/4, 98 pt, 99/1A, 99/2A, 99/1B, 99/2B, 99/2C 99/2D, 99/2F, 99/3A, 99/3B, 100 pt, 101/1A, 101/1B, 101/1C, 101/2, 102/1, 102/2, 102/3, 105/1A, 105/1E, 107/2B, 107/2C, 107/3A, 107/3B, 107/3C, 110/1D, 113/1A, 113/1B, 116/10, 117/pt, 9/pt, 10/pt, 11/pt, 12/pt, 13/pt, 14/pt, 15/pt, 16/pt, 37/pt, 38/pt, 39/pt, 40/pt, 41/pt, 40/1pt, 44/1pt, 48/pt, 49/pt, 50/pt, 52/pt, 110/pt, 111/pt, 114/pt, 103/pt, 113/pt, 115/pt, 109/pt, 99/pt, 85pt

	5
	Total Plot Area
	 10,62,607 m2
	14,54,275 m2

	6
	Total permissible built up area
	13,26,675 m2 ( FSI ),

13,26,675 m2 Construction Built up Area
	14,54,275 m2 (FSI)
19,87,994.46 m2 Construction Built up Area 

	7
	Estimated cost of the project
	Rs.1500.62 Cr.
	Rs. 2568 Cr.

	8
	No of Buildings 
	1 BHK-2400 Units, 2BHK:9786 Units, 3 BHK:1070 Units, Vilas:27, School:2, Hospital 2, and 1 Police Station, Shopping mall, Library, Market, Retail shops Blocks, Public Transport hub, Post Office.
	1 BHK: 10898 Nos.; 2 BHK: 9895 Nos.; 3 BHK: 1028- Nos.; Vilas: 27 Nos.; School: 3, Hospital: 3, Police Chowky: 1, Shopping Mall & Multiplex:1, ,Retail Shops, Public Transport hub, Post office, Cemetery, Fire Staions:2, Social & recreational Facilities with swimming Pools:5, Receiving  Station: 3.

	9
	Water Requirement
	9826CMD, Source: MIDC 1. Fresh Water 5898 CMS
	Water requirement: 15,402 CMD
Source: MIDC
Fresh Water: 10,051 CMD

	10
	Wastewater generated
	7861 CMD,4 STP of Capacity: 1800 CMD, 3000CMD, 2300CMD and 2300CMD capacity Recyeled water will be used for flushing gardening and HVAC water make up.
	Sewage generated: 12,143 CMD
Total capacity of STP: 14,000 CMD

Recyeled water will be used for flushing, gardening and HVAC water make up.

	11
	Rain Water Harvesting
	100 no of recharging pits of 3m x 3m will be provided for rain water harvesting
	202 no of recharging pits of 3m x 3m will be provided for rain water harvesting 

	12
	Solid Waste Generation
	Dry garbage: 22,099 kg/day, Wet garbage: 14,732 kg/day, Biomedical waste: 750 kg/day, STP sludge: 79m3/day
	Dry garbage: 33,924 kg/d
Wet garbage: 22,616 kg/d

	13
	Disposal
	Debris generated will be used for filling of plinth area, site gradation and landscaping. Top Soil will be preserved and later refused in landscaping. Biodegradable waste would be transferred to the composing unit. Non biodegradable waste will be recycled. STP sludge will be used as manure.
	Debris generated will be used for filling of plinth area, site gradation and landscaping. Top Soil will be preserved and later refused in landscaping. Biodegradable waste would be transferred to the composing unit. Non biodegradable waste will be recycled. STP sludge will be used as manure

	14
	Energy
	Power Requirement: during operation phase: 55MW, Source: MSEDCL, DG sets of 19,755 KVA capacity.
	Power Requirement: during operation phase: 79 MW, Source: MSEDCL, DG sets of 26,456 kVA capacity.

	15
	Energy Conservation
	Saving energy by using solar water heating and solar street lighting
	Saving energy by using solar water heating and solar street lighting

	16
	Green Belt Development
	Area for green belt: 3,14,820 sq.m. Nos. of new trees to be planted: 20,340 trees
	Area for green belt: 3,83,570 sq.m. Nos. of new trees to be planted: 24,750 trees

	17
	Traffic Management
	Road, parking and paving area: 3,79,470 sq.m. Parking spaces;9,175 (four wheelers) and 2,700 (two wheelers).
	Two wheelers: 8010 Nos.
Four Wheelers: 15,043 Nos. 

	18
	Evironmental Management Plan
	Total capital cost for EMP shall be Rs.1375 Lakhs and O & M for EMP shall be 76 lakhs The project proponent agreed to maintain O&M of STPs and other EMP.
	Capital Cost: 3680 lakhs
O & M cost: 508 lakh/year

The project proponent agreed to maintain O&M of STPs and other EMP.
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