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Kitchen Setup & Interiors
Kitchens can be classified into 3 types:

a. Pantry Kitchen – Primarily to serve light snacks and drinks.

b. Cafe Kitchen – To serve pre-cooked/lightly cooked food (all meals but limited menu) and drinks.

c. Full-service Kitchen – To cook food from basic raw ingredients with all meals / full menu.

	
	Sales office Kitchen
	Pantry Kitchen
	Cafe Kitchen
	Full-service Kitchen

	Likely Usage
	· All sales offices
	· Clubhouse of small & medium projects
	· Clubhouse of large and very large projects

· Banquet facility with capacity of 150+ shall have attached café kitchen (no additional store) to allow 3rd party catering
	· Full-service restaurant (standalone or in a clubhouse) with seating for min. 100 pax.



	Suggested Size (cannot be more than 10% smaller than this)
	· Area: 60-80 sq. ft.

· Width: ~8 feet
	· Area: 200 sq. feet

· Width ~10 feet

· To be completed along with rest of facility
	· Area: 250 sq. feet (excluding any separate store area)

· Width ~10 feet

· To be completed along with rest of facility (except for equipment which shall follow note below)
	· Area: 600-900 sq. ft. (excluding any separate store area). 

· Space is to be left bare shell (except for the mandatory equipment below) and finished as per operator design once operator is appointed.

	Equipment List 
	1. 2 stove hob

2. Full-size Refrigerator Domestic two door refrigerator 275 lit

3. Sink / washing area
4. Garbage disposal 

5. Exhaust fan with appropriate ventilation

6. Water purification machine (aquaguard type based on direct water supply, assuming there will be a potable water connection; if unlikely to be available, mineral water (50  ltr) dispensing machine)

7. Some storage shelves


	Mandatory:

1. Microwave

2. Hot plate

3. Juicer / blender

4. Full-size Refrigerator- 2 door commercial fridge- 2 nos
5. Sink / washing area
6. Garbage disposal 

7. Exhaust fan with appropriate ventilation

8. Water purification machine (aquaguard type based on direct water supply, assuming there will be a potable water connection; if unlikely to be available, mineral water (50  ltr) dispensing machine)

9. Pop-up Toaster / & Sandwich Griller

10. Storage shelves

11. Salamander

12. Small table top oven
	Mandatory (for club’s main kitchen and banquet kitchen):
1. Large Double Sink / washing area
2. Garbage disposal

3. Exhaust system (fan / chimney)

To be discussed with operator and then finalized (only for club’s main kitchen, not for banquet kitchen):
4. Microwave

5. Hot plate / electric hob- Commercial inductions-4 nos

6. Juicer / blender / Grinder

7. Full-size Refrigerator - 2 door commercial fridge- 3 nos

8. Deep Freezer, Commercial Oven 

9. Water purification machine (aquaguard type based on direct water supply, assuming there will be a potable water connection; if unlikely to be available, mineral water (50  ltr) dispensing machine)

10. Pop-up Toaster / Sandwich Griller

11. Salamander

note: for banquet kitchen, only platform and washing/sink to be provided.
	Mandatory:

1. Gas bank

2. Pot wash / Dish wash area 

3. Exhaust system (fan / chimney)

4. Garbage disposal

To be discussed with operator and then finalized:
5. Hob / Stoves

6. Juicer / blender / Grinder
7. Full-size Refrigerator - 2 door commercial fridge- 3 nos

8. Freezer 

9. Microwave
10. Oven / & Tandoor
11. Bain Marie

12. Water purification machine (aquaguard type based on direct water supply, assuming there will be a potable water connection; if unlikely to be available, mineral water (50  ltr) dispensing machine)

13. Electric Tandoor

14. Pop-up Toaster / Sandwich Griller

15. Others as may be decided with operator

16. Walk-in refrigerator

17. Deep freezer

18. Deep fat fryer



	Estimated staff working inside
	1-2
	2
	3-4
	4+ 8+

	Reference Sample
	
	
	Sales Office @ Lodha Place, Upper Worli

Amara Clubhouse
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	Clubhouse @ Lodha Goldcrest, Lonavala
Lodha Park Club house
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All kitchens should have:

a. Ample storage (preferably with an attached store room for Cafe Kitchens and Full-service Kitchen).

b. Space/provision for staff to sit down when they are not working.

c. Sufficient (if in doubt, extra) sockets/plug points and electrical load.

d. Ample white light / Well-lit. Lux level- 500
e. Nearby location for staff to change.

f. Nearby toilet for staff use.

g. Wet area (sink/washing) located as far away as feasible from gas/hot plate and other electrical equipment.

h. Maximum counter length.

Notes: 

1. Operator to be determined at least 45 days before opening for Pantry Kitchen and Cafe Kitchen and min. 3 months before opening for Full-service kitchen. This operator can be St. Amand or 3rd party.

2. In case of kitchen for banquet hall, we will only provide appliances 1,2 and 3 under ‘Café Kitchen’ and platform. Rest of the cooking equipment shall be brought by the caterer. If St Amand is catering, they will use the main club of the kitchen for most of the cooking.

3. Equipment to be provided by Lodha v. Equipment to be brought by vendor will be determined during commercial negotiation. As far as possible, Lodha to ensure that maximum equipment is brought by the operator (leading to better long-term maintenance). No equipment to be purchased ordered by design/CM, except what is required to be ‘built in’ i.e. installed in permanently fixed location. Any equipment in Lodha scope to be ordered by Hospitality / Admin in consultation with operator; such equipment shall be paid out of Construction budget if ordered prior to or within 3 months of operationalization of the relevant KCA.
4. Equipment capacity and make to be determined in discussion with the operator, based on menu and likely quantum of customers served.
Annexure-1
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