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Marble replacement guidelines for Bellissimo A, B &C
Once possession is given to customer, no marble slab shall be changed by Lodha (except pre-identified ones as per policy below).
Prior to possession, each flat shall be inspected by any one of the following:
1. COO
2. Chief Architect
3. Head – Facility Management
4. Handover Team Representative to project
And they will identify and mark any of the slabs which require replacement (such slabs shall be marked with a red in x with a red non-erasable marked, along with sign and date of the identifying person). All such pre-identified slabs will be replaced by project management no later than 45 days from the date of identification of the slab.
The aforesaid team will use the following guidelines to pre-identify any slabs that need replacement:
1. The marble slab has a distinct breakage or hole in its body (which may or may not have been filled in with a filler material)
2. The edge of the marble slab is chipped off by more than 1 cm
3. The marble slab has a crack of width more than 3 mm (width of crack to be seen, not width of filled up line after crack)
4. If there is a shade variation which is visually apparent and significantly aesthetically displeasing and located in a prominently visible location
When possession is handed over to customer, FM / CC will explain that ‘as part of our rigorous quality control process, the flat has been inspected by internal and external experts on multiple occasions. At time of final inspection, certain slabs of marble (identified as above), on account of their natural flaws, have been found to be not meeting our quality standards and hence, we shall replace them within the next 45 days at our own cost to ensure that all units meet our stringent quality norms.’
In case of ferrous stains on the marble, FM shall offer to have the same bleached on one occasion but also simultaneously explain ‘that same has occurred on account of natural characteristics of marble and its reaction with other materials and is a part of the natural settling process’
This policy shall also serve as the guideline for quality control / replacement for all locations where the company provides natural marbles.
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