List of Requirements for EC
1. User Details 

2. Details required for EC
	Sr. No. 
	Description
	Details
	Unit

	1
	Plot Area
	Project Proponent
	m2

	2
	FSI Area 
	Project Proponent
	m2

	3
	Non FSI Area 
	 Break up of Non FSI like Stilt, Passages, balcony, Podium, Lift and any other covered area not counted in FSI by Project Proponent
	m2

	4
	Total Construction Area 
	Project Proponent
	m2

	5
	Building Confg. & Height 
	Project Proponent
	m

	6
	No. of tenements & shops 
	Total Flats: --- Nos. ( 1BHK ---, 2 BHK---, 3BHK ---,4 BHK---), Shops: -- Nos. Office:----- m2  
Project Proponent
	Nos. 

	7
	Total Population
	Pristine
	Nos. 

	8
	Water requirement 
	Pristine
	KLD

	9
	Sewage generation 
	Pristine
	KLD

	10
	STP Capacity and STP technology
	Pristine
	-

	11
	STP Location
	Preferably open to sky or at least 40% area open to sky
	-

	12
	Total Solid waste generation
	Pristine
	kg/day

	13
	Total RG Area provided
	RG required: -------- m2 & RG provided: ----- m2
(Ground: ----- m2 & Podium: ----- m2)  
No of Trees on site----nos, 
Trees to be cut ---- nos, 
Trees to be transplanted ---- nos, 
New trees to be planted----nos
Project Proponent
	m2

	14
	Power requirement 
	Connected load: ---- MW, Demand load: ---- MW Project Proponent
	MW

	15
	Energy efficiency 
	
(Solar: ---) at least 10%
	%

	16
	D.G. Set Capacity 
	1 x --- kVA, 1 x --- kVA Project Proponent
	kVA

	17
	Parking (4 W) & (2 W)
	4 W: -----
2 W: ----
Charging points: ---- Project Proponent
	Nos. 

	18
	RWH Tank Capacity 
	Terrace area of buildings, rest calculations from Pristine
	m3

	19
	Project Cost 
	--- Cr Project Proponent
	Rs. 

	20
	EMP Cost
	Capital Cost : ---- Lakh,  O&M: ----- Lakh/yr  Pristine
	Rs. 

	21
	Plan
	Conceptual Plan/approved plan/LOI along with proforma Project Proponent
	

	21
	Site contour
	Contour Plan with details of nalla if any  Project Proponent
	

	22
	Site photo
	Site photograph from 4 sides of the plot Project Proponent
	

	23
	Demolition details
	Quantity of demolition waste if old structures are to be demolished  Project Proponent
	

	24
	Google image 
	Google image of site along with plot boundary superimposed on it  Project Proponent
	

	24
	Scrutiny fees 
	If project cost:
1. upto 50Cr	: 1.5 Lakh
2. 50 -100 	:  4 Lakh
3. 100-500 	:  7 Lakh
4. 500 – 1000 	:  15 Lakh
5. Above 1000 cr	:  30 Lakh
Account Name and No. ----
	



3. MPCB Consent Registration details

[bookmark: _GoBack]1. Authority letter (On Company Letterhead)
2. PAN Card of Industry 
3. Industry Registration Certificate 
4. PAN Card of Authorized person 
5. List of directors of Company (On Company Letterhead)
6. Aadhar card of Authorized person
Pristine Consultants
