M/s. Acme Housing India Pvt. Ltd.

FORM I

FORM-I
(I) Basic Information

	Sr. No.
	Item
	Details

	1
	Name of the Project
	Environment Clearance of Terms of Reference for Amendment in “Acme Ozone” Residential cum Commercial project under Rental Housing Scheme at Land bearing Gut. No. 61/1/1, Gut. No. 61/1/2, 3, 4, 61/2/1, 2, 3, Village - Chitalsar-Manpada, Tal. & Dist. Thane, by M/s. Acme Housing India Pvt. Ltd.

	2
	S. No. in the Schedule
	8(b) Building and Construction Projects

	3
	Proposed capacity/area /length/tonnage to be handled/command area/lease area/ number of wells to be drilled
	Environment Clearance received File F.No. SEAC-2014/CR-234/TC-1 dated 28th January 2016.
· Plot Area:          54500 sqm
· Total BUA:       361836.04 sqm

Completed development consisting of 8 no’s buildings in plot A, 2 no’s buildings in plot B, 6 no’s buildings in MMRDA.


	
	
	Proposed expansion:
Plot Area:    54500.00 sqm
Total BUA: 383199.01 sqm
Proposed FSI: 176510.99 sqm
Proposed Non FSI: 206688.02 sqm
For the configuration of –

Building Name & number
Number of floors
Height of the building (Mtrs)
Plot A - Alpinia building no 1
3 lvl Podium (Gr.+2P)
+Stilt+FAS+1st -26th Floor
91.80
Plot A - Basilia building no 2
3 lvl Podium (Gr.+2P)
+Stilt+FAS+1st -26th Floor
91.80
Plot A - Centilia builiding no 3
3 lvl Podium (Gr.+2P)
+Stilt+FAS+1st -26th Floor
91.80
Plot A - Dandelia building no 4
3 lvl Podium (Gr.+2P)+Stilt+FAS+1st -26th Floor
91.80
Plot A - Eucalyptia building no 5
2 lvl Basement + 3lvl Podium(Gr.+2P)+Stilt+1st- 19th floor+Fire Check floor+ 20th- 36th(Pt) floors
121.77
Plot A - Fenelia building no.6
2 lvl Basement+ Gr(Pt.)/ 1st lvl . Podium +Mezzanine(Pt.)/2nd lvl Podium+3rd Podium +Stilt + 1st to 19th floor

+fire Check Floor +20th -36th (Pt) floor
121.77
Plot A - Gingelia building no.7
1lvl Basement+ Gr(Pt)/1st lvl Podium +1st Floor (Pt.)/2nd lvl Podium+ 3rd lvl Podium (Gr.+2P)+ Stilt +FAS+ 1st-26th floors
91.80
Plot A - Herbelia building no.8
3 lvl              Podium(Gr.+2P)+Stilt+FAS+1st
-26thFloor
91.80
Plot B - Oakwood
3P(Gr.+2P)+St+28 Floors
90.95
Plot B - Ashwood
3P(Gr.+2P)+St+28 Floors
90.95
MMRDA - building no.1
Gr/Shops+25th Floor
76.30
MMRDA - building no. 2
Stilt+25th Floor
76.30
MMRDA - building no. 3
Gr./Shop+22nd Floor
67.60
MMRDA - building no. 4
Gr./Shop+22nd Floor
67.60
MMRDA - building no. 5
Stilt+23rd Floor(part)
70.50
MMRDA - building no. 6
Gr./Shop+22nd Floor
67.60


	4
	New/Expansion/Modernization
	Expansion in existing Project- 
Environment Clearance received File F. No. SEAC-2014/CR-234/TC-1 dated 28th January 2016 for Total BUA:       361836.04 sqm 

	5
	Completed Capacity/Area etc.
	PLOT A Building no. 2 & 3 Possession given Building no.1,4,7,8 Under Construction Building no.5 & 6 Work not yet started Plot B Oakwood & Ashwood Possession Given MMRDA Building no.1,2,5 &6 Under finishing stage Building no.3 & 4 OC received.

	6
	Category of Project i.e. ‘A’ or ‘B’
	‘B’


	7
	Does it attract the general condition? If Yes, Please specify
	No

	8
	Does it attract the specific condition? It yes, Please specify
	Not Applicable

	9
	Location 
	Village - Chitalsar-Manpada, Tal. & Dist. Thane

	
	Plot/Survey/Khasra No.
	Land bearing Gut. No. 61/1/1, Gut. No. 61/1/2, 3, 4, 61/2/1, 2, 3, Village - Chitalsar-Manpada, Tal. & Dist. Thane

	
	Village
	Chitalsar-Manpada

	
	Tehsil
	 Thane 



	
	District
	 Thane 



	
	State
	Maharashtra 

	10
	Nearest railway station/airport along with distance in kms.
	Thane Railway Station. (Aerial distance : 2.8 Km towards East) 



	11
	Nearest Town, City, District Headquarters along with distance in kms.
	Thane Municipal Corporation. (5.5 km)


	12
	Village Panchayats, Zilla Parishad, Municipal Corporation, Local body (complete postal addresses with telephone nos. to be given)
	Thane Municipal Corporation. 
Mahapalika Bhavan, Chandan Wadi, Mahapalika Bhavan Rd, PanchPakhadi, Thane West, Thane, Maharashtra 400602.

	13
	Name of the applicant
	Mr. Munish P. Doshi 



	14
	Registered Address
	Ascent Constructions Pvt. Ltd
 GladyAlwares Road, Near Khewra Circle, Manpada, Thane-400 607. 



	15


	Address for correspondence:
	Same as above

	
	Name
	Mr. Munish P. Doshi

	
	Designation(Owner/Partner/CEO)
	Owner

	
	Address
	As Above

	
	Pin Code
	400 055

	
	E-mail
	munish@acmehousing.com and pina@acmehousing.com

	
	Telephone No.
	+91 67570000

	
	Fax No.
	+91 26710976

	16
	Details of Alternative Sites examined, If any.

Location of these sites should be shown on a topo sheet.
	Not Applicable

	17
	Interlinked Projects
	Not Applicable.

	18
	Whether separate application of interlinked project has been submitted?
	Not Applicable

	19
	If yes, date of submission
	Not Applicable

	20
	If no, reason
	Not Applicable

	21
	Whether the proposal involves approval/clearance under:
The Forest (Conservation) Act, 1980?

The Wildlife (Protection) Act, 1972?

The C.R.Z. Notification, 1991? 

 if yes, details of the same and their status to be given.
	No

	22
	Whether there is any Government Order/Policy relevant/relating to the site?
	No

	23
	Forest land involved (hectares)
	No



	24
	Whether there is any litigation pending against the project and/or land in which the project is propose to be set up?

Name of the Court

Case No.

Orders/directions of the Court, if any and its Relevance with the proposed project.
	No


* Capacity corresponding to sectoral activity (such as production capacity for manufacturing, mining lease area and production capacity for mineral production, area of mineral exploration, length for linear transport infrastructure, generation capacity for power generation etc.)
(II) Activity

1. Construction, operation or decommissioning of the Project involving actions, which will cause physical changes in the locality (topography, land use, changes in water bodies, etc.)

	Sr. No.
	Information/Checklist Confirmation
	Yes/No
	Details thereof (with approximate quantities/ rates, wherever possible) with source of information data

	1.1
	Permanent or temporary change in land use, land cover or topography including increase in intensity of land use (with respect to local land use plan)
	No
	The project is for expansion. There will be no change in the land use. The planning is as per local land use plan.

	1.2
	Clearance of Completed land, vegetation and building?
	No
	Total number of trees to be planted: 633 no’s


	1.3
	Creation of new land uses:
	No
	Not Applicable

	1.4
	Pre-construction investigations e.g. bore houses, soil testing?
	Yes
	Geotechnical investigations have been carried out.

	1.5
	Construction Works?
	Yes
	PLOT A Bldg no. 2 & 3 Possession given Bldg no.1,4,7,8 Under Construction Bldg no.5 & 6 Work not yet started Plot B Oakwood & Ashwood Possession Given MMRDA Bldg no.1,2,5 &6 Under finishing stage Bldg no.3 & 4 OC received

	1.6
	Démolition Works?
	No
	Not Applicable 

	1.7
	Temporary sites used for construction works or housing of construction workers?
	Yes
	· During the construction phase about 70 to 80 no’s of Labors will be provided with temporary housing facilities. 

· The site will have temporary sheds during construction phase, which will be later dismantled.

	1.8
	Above ground buildings, structures or earthworks including linear structures, cut and fill or excavations.
	Yes
	Building Name & number
Number of floors
Height of the building (Mtrs)
Plot A - Alpinia building no 1
3 lvl Podium (Gr.+2P)
+Stilt+FAS+1st -26th Floor
91.80
Plot A - Basilia building no 2
3 lvl Podium (Gr.+2P)
+Stilt+FAS+1st -26th Floor
91.80
Plot A - Centilia builiding no 3
3 lvl Podium (Gr.+2P)
+Stilt+FAS+1st -26th Floor
91.80
Plot A - Dandelia building no 4
3 lvl Podium (Gr.+2P)+Stilt+FAS+1st -26th Floor
91.80
Plot A - Eucalyptia building no 5
2 lvl Basement + 3lvl Podium(Gr.+2P)+Stilt+1st- 19th floor+Fire Check floor+ 20th- 36th(Pt) floors
121.77
Plot A - Fenelia building no.6
2 lvl Basement+ Gr(Pt.)/ 1st lvl . Podium +Mezzanine(Pt.)/2nd lvl Podium+3rd Podium +Stilt + 1st to 19th floor

+fire Check Floor +20th -36th (Pt) floor
121.77
Plot A - Gingelia building no.7
1lvl Basement+ Gr(Pt)/1st lvl Podium +1st Floor (Pt.)/2nd lvl Podium+ 3rd lvl Podium (Gr.+2P)+ Stilt +FAS+ 1st-26th floors
91.80
Plot A - Herbelia building no.8
3 lvl              Podium(Gr.+2P)+Stilt+FAS+1st
-26thFloor
91.80
Plot B - Oakwood
3P(Gr.+2P)+St+28 Floors
90.95
Plot B - Ashwood
3P(Gr.+2P)+St+28 Floors
90.95
MMRDA - building no.1
Gr/Shops+25th Floor
76.30
MMRDA - building no. 2
Stilt+25th Floor
76.30
MMRDA - building no. 3
Gr./Shop+22nd Floor
67.60
MMRDA - building no. 4
Gr./Shop+22nd Floor
67.60
MMRDA - building no. 5
Stilt+23rd Floor(part)
70.50
MMRDA - building no. 6
Gr./Shop+22nd Floor
67.60


	1.9
	Underground works including mining or tunneling?
	Yes 
	No underground works including mining / Tunneling is required except minor activities like excavation of earth only for basement, foundation, lay down of pipes, underground storage tank, electric cables, mobile STPs etc.

	1.10
	Reclamation works?
	No
	-

	1.11
	Dredging?
	No
	-

	1.12
	Offshore structures?
	No
	-

	1.13
	Production and manufacturing Process?
	No
	-

	1.14
	Facilities for storage of goods or materials?
	Yes
	Separate raw material storage yard will be made, which will be temporary. 
Construction Phase:

· Cement will be separately stored under cover in bales.

· Sand will be stacked neatly under tarpaulin cover.

· Bricks and steel will be laid in open.

Operation  Phase:

Storage area for Manure and Sludge will be provided.

	1.15
	Facilities for treatment or disposal of solid waste or liquid effluents?
	Yes
	Construction Phase:

Construction waste generated shall be properly disposed off as per the municipal laws. The necessary metal and recyclable waste shall be sold to vendors for recycling.

The solid waste generated by the onsite workers shall be handed over to municipal authority for safe disposal.
Operation Phase:
The Total solid waste generation for the entire project will be 10816 kg/day.

Dry waste

4380 kg/day

Wet waste

6436 kg/day

This will be treated/disposed off as per following:
· The biodegradable waste will be processed in OWC. 

· Maximum requirement of manure for gardening will be used.

· Non- Biodegradable waste will be handed over to recyclers.

· Sludge Quantity (dry): Sewage sludge will be used as manure for gardening

· Total 2445 KLD waste water will be generate it will treated in STP of capacity 1160 KLD. 
STP technology: MBBR

Sewage generation:


Plot A: 1015 KLD

Plot B: 270 KLD

MMRDA: 1160 KLD

Capacity of STP:


Plot A: 1015 KLD

Plot B: 270 KLD

MMRDA: 1160 KLD

	1.16
	Facilities for long term housing of operational workers?
	No
	No, There shall be no facilities for long term housing of operational workers

	1.17
	New road, rail or sea traffic during construction of operation?
	No
	There will be no new road and rail.

	1.18
	New road, rail, air, waterborne or other transport infrastructure including new or altered routes and stations, ports, airports etc.?
	No
	NA

	1.19
	Closure or diversion of Completed transport routes or infrastructure leading to changes in traffic movements?
	No
	There will be no diversion or closure of the Completed transport routes and infrastructure. 

	1.20
	New or diverted transmission lines or pipelines?
	No
	There will be no shifting of electrical transmission line. But the project involves construction of new internal pipelines for fresh water, recycled water, rain water harvesting, sewer lines and internal power distribution lines. 

	1.21
	Impoundment, damming, culverting, realignment or other changes to the hydrology of watercourses or aquifers?
	No
	-

	1.22
	Stream crossings?
	No
	-

	1.23
	Abstraction or transfers of water from ground or surface waters?
	No
	Construction Phase:
Water requirement in the construction phase will be supplied depending upon construction activity is 25 KLD will be fulfilled by private tanker water. 
Operation Phase:
Domestic water req. shall be served by TMC water supply & flushing and landscaping water requirement shall be done by onsite STP treated water

	1.24
	Changes in water bodies or the land surface affecting drainage or run-off
	No
	There will be no change in the drainage pattern. 

	1.25
	Transport of personnel or materials for construction, operation or decommissioning?
	Yes
	Construction:

There will be movement of personnel’s, materials and machineries during the construction phase. The impact due to the same will be negligible as local people will be deployed and the construction material and machinery required will be mobilized from the local area. Thus there will be contribution of marginal noise & vehicular emissions.
Post Construction:

During commissioning, there will be transportation of personnel’s and materials in and out of the project regularly. The Completed roads will be utilized for the transportation of material and personnel.

	1.26
	Long-term dismantling or decommissioning or restoration works?
	No
	Restoration works for the project on long term will be an ongoing activity which will not have any impact on physical environment.

	1.27
	Ongoing activity during decommissioning which could have an impact on the environment?
	No
	There is no decommissioning activity.

	1.28
	Influx of people to an area in either temporarily or permanently?
	Yes
	Construction Phase

During the construction phase about 70 to 80 no’s Labors will be provided with housing facilities which will be purely in temporary basis and during peak hours remaining will be deployed from nearby places.

Operation Phase

On completion of the project, there will be regular movement of residents, visitors, staff and related personals. 
Plot A = 7693, Plot B = 2300, MMRDA = 12504 (12534-30_6flats min) 
Total: 22399 No’s

	1.29
	Introduction of alien species?
	No
	Indigenous or Natural species will be planted.



	1.30
	Loss of native species or genetic diversity?
	No
	Not applicable

	1.31
	Any other actions?
	No
	Not applicable




2.
Use of Natural resources for construction or operation of project (such as land, water, materials or energy, especially any resources which are non-renewable or in short supply).
	Sr. No.
	Information/Checklist Confirmation
	Yes/No
	Details thereof (with approximate quantities/ rates, wherever possible) with source of information data

	2.1
	Land specially undeveloped or agricultural land (ha)
	No
	The plot land is non agricultural type.



	2.2
	Water (expected source & competing users) unit KLD
	Yes
	Construction Phase:
 It is expected to house about 70 to 80 labours at site.
Operation phase:

The water requirement will be met by the TMC/Recycled water from STP
Total

· Fresh water: 1980 KLD

· Source: TMC
· Recycled water: 
Total: 3116 KLD 

Flushing: 1062 KLD, 
Gardening: 72 KLD 

	2.3
	Minerals (MT)
	No 
	-


	2.4
	Construction material – stone, aggregates, and/soil (expected source-MT)
	Yes
	The construction materials, which will be used in the project site, will be procured from authorized local dealer

	2.5
	Forests and timber (source-MT)
	Yes
	For Apartments timber doors will be used. Certified wood to be used.

	2.6
	Energy including electricity and fuels (source, competing users) Unit: fuel (MT), energy (KW)
	Yes
	Power requirement: 

(a) Construction Phase: 100 kVA
(b) Operation Phase:
· Connected load : 
Plot A: 28176 kW,

Plot B: 2833 kW,

MMRDA: 14955 kW

Total Connected load: 45964 kW
· Demand load:  

Plot A: 9735 kW,

Plot B: 1503 kW,

MMRDA: 5144 kW

Total Connected load: 16382 kW

· Fuel used: HSD
· Common area lighting, street lighting and landscape lighting on LED

· Use of electronic ballast instead of copper ballast

· Providing timers for common area lighting

· Use of hydro- pneumatic pumping system/ventilation & lifts with VFD drives and soft starter

· Use of BEE star rated pumps

· Use of APFC panels0

· Use of solar water heater panels

Provision of Solar system for Common area lighting, street lighting and landscape lighting

Source of power supply:
M.S.E.D.C.L
Number and capacity of DG sets to be used: 
Plot A: 2NOS. Capacity: 630 KVA & 1 No of 500 KVA,

Plot B: 1 NO. Capacity: 500 KVA, MMRDA: 2 NOS. Capacity: 630 KVA

	2.7
	Any other natural resources (use appropriate standard units)
	No
	No other natural resources will be used.


3. Use, storage, transport, handling or production of substances or materials, which could be harmful to human health or the environment or raise concerns about actual or perceived risks to human health

	Sr. No.
	Information/Checklist Confirmation
	Yes/No
	Details thereof (with approximate quantities/ rates, wherever possible) with source of information data

	3.1
	Use of substances or materials, which are hazardous (as per MSIHC rules) to human health or the environment (flora, fauna, and water supplies)
	Yes
	Each DG set shall be provided with proper acoustic enclosure. 

Oil spillage from construction machinery & vehicles, discarded containers of paints solvents etc, tarpaulins, etc. Hazardous waste will be management as per the rules. 

	3.2
	Changes in occurrence of disease or affect disease vectors (e.g. insect or water borne diseases)
	No
	During the entire construction phase adequate precaution will be taken to avoid stagnation of water giving rise to mosquito breeding. Further, storm water network will be well designed to leave no stagnant water pockets, at any point of time. The storm water line will not cross wastewater line. Proper housekeeping practices will be adopted.

	3.3
	Affect the welfare of people e.g. by changing living conditions?
	Yes
	Positive impact due to enhanced and hygienic living conditions. Aesthetic value of area will be improved. It will provide employment opportunities to the local people in terms of skilled and unskilled labour during construction and service personnel during operational phase.

	3.4
	Vulnerable groups of people who could be affected by the project e.g. hospital patients, children, the elderly etc.,
	No
	There are no vulnerable areas within 1.0 km from the site. 

	3.5
	Any other causes
	No
	No other causes identified.




4. Production of solid wastes during construction or operation or decommissioning (MT/month)

	Sr. No.
	Information/Checklist Confirmation
	Yes/No
	Details thereof (with approximate quantities/ rates, wherever possible) with source of information data



	4.1
	Spoil, overburden or mine wastes
	No
	There is no activity which may generate spoil, overburden & mine waste.


	4.2
	Municipal waste (domestic and or commercial wastes)
	Yes
	The solid waste management facility will be proposed as per MSW rules. Garbage will be collected manually from each of the building in the garbage collection room. The garbage collected from area will be segregated into wet and dry garbage. 

Operation Phase:

Dry waste

 4380 kg/day

Wet waste

6436 kg/day

Treatment & Disposal : 

· The biodegradable waste will be processed in OWC.

· Non- Biodegradable waste will be handed over to recyclers.
Dry sewage sludge will be used as manure for gardening.

	4.3
	Hazardous wastes (as per hazardous waste management rules)
	Yes
	Used oil from DG set will be stored carefully at separate location duly marked and will be sold to CPCB authorized recyclers. The mercury containing lamps will not be used in the post construction phase. However, the other hazardous waste such as waste tube lights, CFL’s, batteries (inverters), will be generated and will be sold to the registered actual users.

	4.4
	Other industrial process wastes
	No
	Not Applicable



	4.5
	Surplus product
	No
	Not Applicable



	4.6
	Sewage sludge or other sludge from effluent treatment
	Yes
	Dewatered / dried sludge from STP 122 kg/day will be used as manure for gardening/ landscaping.

	4.7
	Construction or demolition wastes
	Yes
	Solid waste during the construction phase would comprise mainly of excavated earth, concrete debris, steel scrap, scrap from insulation material for air-conditioning and packaging material. 

Cement bags, waste paper and cardboard packing material will be sold off to recyclers. Unusable steel scrap will also be collected at site and sold to recyclers.

Excavated soil and rubble will be used for back filling and remaining material will be disposed by Covered trucks to the authorized sites.

	4.8
	Redundant machinery or equipment
	No
	All equipments used for the construction will be maintained on regular basis.

	4.9
	Contaminated soils or other materials
	No
	No contaminated soil found.



	4.10
	Agricultural wastes
	No
	No 

	4.11
	Other solid wastes
	No
	No 


5. Release of pollutants or any hazardous, toxic or noxious substances to air (kg/hr)

	Sr. No.
	Information/Checklist Confirmation
	Yes/No
	Details thereof (with approximate quantities/ rates, wherever possible) with source of information data

	5.1
	Emissions from combustion of fossil fuels from stationary or mobile sources
	Yes
	· Exhaust emission generated from Auto mobiles will be checked by proper PUC certificate.

· Stationary machine like DG set will be properly maintained to reduce air pollution.

	5.2
	Emission from production processes
	No
	There is no production as the proposed project is residential cum commercial complex.

	5.3
	Emissions from materials handling including storage or transport
	Yes
	· Emissions will be generated, while handling and transportation of materials like cement, sand etc. to site, will be temporary in nature.
· Regular water sprinkling & tarpaulin covers will be provided to cover dust emissions.

	5.4
	Emissions from construction activities including plant and equipment
	Yes
	The project may cause rise in dust levels during construction phase. Precautions will be taken to reduce dust generation during construction phase.
· Mixed use will eliminate the handling of cement, sand and concrete thus dust emission will be minimized.

· Mixed use will also reduce the trucks trips.

· Tarpaulins will be used to cover trucks carrying debris.

· Water sprinkling will be done at regular intervals to reduce control of dust generation.

	5.5
	Dust or odours from handling of materials including construction materials, sewage and waste
	Yes
	Construction Phase:

Dust and odour  generation due to

· Movement of vehicles 

· Material handling and storage.

· Solid waste disposal.

· Black water disposal.
Mitigation measures:

· Sprinkling water on unpaved roads.

· Covering materials storage shed with tarpaulin sheet or G.I metal sheets to reduce dissipation of dust to surrounding.

· Solid waste shall be collected at a designated location away from the working area for disposal and collection by municipal authority.

· The liquid waste shall be collected from the isolated mobile STP and collected by municipal authority.
Operation Phase:

· Odour generation due to disposal of sewerage.
· Emissions will be generated from operation of DG sets in emergency cases.
Mitigation measures:
· MBR technology shall be used which an efficient STP methodology and results in lower odor generation. 

· The STP shall be naturally and mechanically ventilated for dispersion of odor and harmful gases.
· The D.G set selected shall be as per CPCB norms w.r.t noise and emission standards.

· The D.G. Set  stack height shall be as per CPCB norms

	5.6
	Emissions from incineration of waste


	No
	Not Applicable.

	5.7
	Emissions from burning of waste in open air (e.g. slash materials, construction debris)
	No
	No such practices shall be entertained.

	5.8
	Emissions from any other sources


	No
	Not Applicable.


6. Generation of Noise and vibration, and emissions of Light and heat

	Sr. No.
	Information/Checklist Confirmation
	Yes/No
	Details thereof (with approximate quantities/ rates, wherever possible) with source of information data

	6.1
	From operation of equipment e.g. engines, ventilation plant, crushers
	Yes
	Noise generation from construction equipment’s used for drilling, cutting operations.

During Operation Phase, Noise will be generated due to operation of DG sets.

For control of noise following measures shall be adopted:

· Properly maintained equipment’s with mufflers will be used.

· High noise generating construction activities would be carried out only during day time.

· Workers working near high noise construction machinery would be provided with ear muffs/ear plugs.

	6.2
	From industrial or similar processes
	No
	  Not Applicable

	6.3
	From construction or demolition
	Yes
	The construction noise will be localized, intermittent in nature. The construction activities will include the following noise generating activities ;

1.  Excavation activities etc.
2.  Concreting and mixing.

3.  Heavy vehicle movement.

4.  Operation of D.G sets.

Following precautions shall be taken to control noise pollution :

· High noise generating construction activities would be carried out only during day time.
· Installation, use and maintenance of mufflers on equipment.
· Workers working near high noise construction machinery would be supplied with ear plugs.

	6.4
	From blasting or piling
	Yes
	Piling foundation is proposed

	6.5
	From construction or operational traffic
	Yes
	Construction phase:

There will be transport of materials for construction work. Precautions will be taken to reduce the impact of the vehicular movement such as vehicular trips will not be at peak traffic hours.

Operation Phase:

· The vehicular parking will be restricted only in the adequate parking area provided, which would help in reducing noise pollution due to traffic congestion.

· Local native plants will be used in plantation which will help to reduce the impact of air and noise pollution.

	6.6
	From lighting or cooling systems
	No
	Not Applicable



	6.7
	From any other sources 
	No
	Not Applicable.




7.  Risks of contamination of land or water from releases of pollutants into the ground or into sewers, surface waters, groundwater, coastal waters or the sea

	Sr. No.
	Information/Checklist Confirmation
	Yes/No
	Details thereof (with approximate quantities/ rates, wherever possible) with source of information data

	7.1
	From handling, storage, use or spillage of hazardous materials
	No
	Not Applicable.

	7.2
	From discharge of sewage or other effluents to water or the land (expected mode and place of discharge)
	No


	The total wastewater generated will be 2445 KLD 

	7.3
	By deposition of pollutants emitted to air into the land or into water
	No
	Dust will be generated during construction phase from earthworks and movement of vehicles. Appropriate dust control measures, including water sprinkling of exposed areas and dust covers for trucks, will be provided to minimize any impacts. DG exhaust will be discharged at stipulated height by providing adequate stack height to the DG sets.

	7.4
	From any other sources
	No
	No 

	7.5
	Is there a risk of long term buildup of pollutants in the environment from these sources?
	No
	No 


8. Risk of accidents during construction or operation of the project, which could affect human health or the environment

	Sr. No.
	Information/Checklist Confirmation
	Yes/No
	Details thereof (with approximate quantities/ rates, wherever possible) with source of information data

	8.1
	From explosions, spillages, fires etc from storage, handling, use or production of hazardous substances
	No
	Each DG set shall be provided with proper acoustic enclosure. Fire Fighting System will be provided.

	8.2
	From any other causes
	Yes 
	There is a risk of accident during construction however proper safety measures will be taken.

	8.3
	Could the project be affected by natural disasters causing environmental damage (e.g. floods, earthquakes, landslides, could burst etc)?
	No
	The project falls under seismic zone-III as per IS1893 (Part-1):2002. The structural design shall be accordingly performed. Hence, no risk due to natural hazards is envisaged.


9. Factors which should be considered (such as consequential development) which could lead to environmental effects or the potential for cumulative impacts with other Completed or planned activities in the locality

	Sr. No.
	Information/Checklist Confirmation
	Yes/No
	Details thereof (with approximate quantities/ rates, wherever possible) with source of information data

	9.1
	Lead to development of supporting, utilities, ancillary development or development stimulated by the project which could have impact on the environment e.g.:
Supporting infrastructure (roads, power supply, waste or waste water treatment, etc)

Housing development

Extractive industries

Supply industries

Other
	Yes
Yes
Yes
No

No
No
	Supporting and ancillary development will take place.

Internal Roads, Rainwater Harvesting, STP etc. will be provided.

The project provides well residential housing area for the occupants
-

-

-

	9.2
	Lead to after use of the site, which could have an impact on the environment
	No
	Not applicable 

	9.3
	Set a precedent for later developments
	Yes
	This will create job opportunity for support staff like security, maintenance, household workers etc

	9.4
	Have cumulative effects due to proximity to other Completed or planned projects with similar effects.
	Yes 
	Impacts on water availability, storm water drainage, availability of electricity, traffic congestion etc.


(iii) Environmental Sensitivity

	Sr. No.
	Areas
	Name/

Identity
	Aerial distance (with 15-km) Proposed project location boundary

	1
	Areas protected under international conventions, national or local legislation for their ecological, landscape, cultural or other related value
	No
	Nil

	2
	Areas which are important or sensitive of ecological reasons – wetlands, water courses or other water bodies, coastal zone, biospheres, mountains, forests
	No
	Nil

	3
	Areas used by protected, important or sensitive species of flora or fauna for breeding, nesting, foraging, resting, over wintering, migration.
	No
	Nil

	4
	Inland, coastal, marine or underground waters

	No
	Nil

	5
	State, national boundaries
	No
	The project is located within Municipal limits.

	6
	Routes or facilities used by the public for access to recreation or other tourist, pilgrim areas
	No
	Not Applicable.

	7
	Defense installations
	No
	No defense installation in the neighborhood.

	8
	Densely populated or built-up area
	No
	Residential, Commercial area all around the site. As per the provision of DCR

	9
	Areas occupied by sensitive man made land uses (hospitals, schools, places of worship, community facilities)
	Yes 
	Schools, hospitals and small temples are observed in 10 km radius.
Site
Distance from the proposed project
(KM/Aerial KM)
Railway Station
Thane Railway station.
5.8 km
Bus Station
Manpada Bus Station

0.41 km
Hospital
Metro Hospital

0.42 km
School
Vasant Vihar High School & Jr. College

1.28 km
College
N G Bedekar College of Commerce 

0.81 km


	10
	Areas containing important, high quality or scarce resources (ground water resource, surface resources, forestry, agriculture, fisheries, tourism, minerals)
	No
	The project will meet water from TMC for its use after proper permissions are obtained.



	11
	Areas already subjected to pollution or environmental damage. (those where Completed legal environmental standards are exceeded)
	No
	All parameters of Air, water and Noise etc. will be maintained within the permissible limit.



	12
	Areas susceptible to natural hazard which could cause the project to present environmental problems

(earthquakes, subsidence, landslides, erosion, flooding or extreme or adverse climatic conditions)
	No
	This area is generally plain& come under seismic zone –III according to Indian Standard Seismic zoning map.




(b) The following shall be inserted at the end, namely:-

“I hereby given undertaking that the data and information given in the application and enclosures are true to the best of my knowledge and belief and I am aware that if any part of the data and information submitted is found to be false or misleading at any stage, the project will be rejected and clearance give, if any to the project will be revoked at our risk and cost.”

Date: 

Place: Mumbai
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