
TO WHOM SO EVER IT MAY CONCERN

M/s Macrotech Developers Limited (hereinafter referred to as the Company) is developing the “Lodha Acme Ozone” project at Mumbai, Maharashtra. The project is aiming to achieve desired rating under the IGBC Green Homes v3 rating System.
The company declares the following:
1. The construction works not started at the site and company ensure that the Basic Facilities for Construction Workforce and the Green Education and Awareness will be implemented at site as per IGBC requirement.
2. The company will ensure that the water fixtures used in the project are as per following flow rates -
	S.No
	Fixture
	Proposed rate 
(Metric units)
	Proposed 
Make
	Proposed Model

	1
	Water Closet 
	4/2 LPF
	Jaquar
	1085G

	2
	Lavatory Faucets
	4.1 LPM
	Jaquar
	6047GD

	3
	Kitchen Faucets
	4.1 LPM
	Jaquar
	6047GD

	4
	Showerhead
	6 LPM
	Jaquar
	1709GA

	5
	Health Faucet
	6 LPM
	Jaquar
	583NGA
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3. The company will ensure that the Lighting Power Density (LPD) used in the project atleast 30% less than baseline Lighting Power Density (LPD) as mentioned below -
	S.No
	Space Description
	Baseline Lighting Power 
Density (LPD)

	1
	Interior Lighting (for Non-residential)
	0.46 W/sq.ft.

	2
	External Lighting
	0.23 W/sq.ft.

	3
	Common Area Lighting
(excluding parking area)
	0.37 W/sq.ft.

	4
	Parking Area
	0.23W/sq.ft.


4. The efficient glass will be used in the project and below mentioned glass parameters considered.
· U-Value: 2.8 W/m2K
· SHGC: 0.59
· VLT: 60%
   

Regards

Authorized Signatory

