BOQ FOR GEOTECHNICAL INVESTIGATION FOR 
PROPOSED ASPI BUILDING IN PASEO CLUSTER, SECTOR 3, PALAVA II
	SR

NO.
	DESCRIPTION OF ITEM
	ESTIMATED QUANTITY
	UNIT
	RATE
	AMOUNT (RS.)

	1
	Mobilization of drilling equipments, accessories, personnel, etc. to site, and demobilization of the same after completion of work as per specifications, contract requirements and instructions of Engineer-in-charge.
	1
	Rigs
	
	

	2
	Setting and shifting of rig at borehole locations 
	3
	Nos.
	
	

	3
	Boring minimum 100mm diameter hole in all kind of soils, fill, soft rock (CR<10%) as per specifications and instructions of Engineer-in-charge.
	40
	RM
	
	

	4
	Coring in rock (N>50, CR>10%) using NX size single tube core barrel and diamond bit.(Min. 3.0m in hard rock)
	12
	RM
	
	

	5
	Conducting Standard Penetration Tests (SPT) in soil at a vertical interval of 1.5m and collecting/preserving SPT soil samples.
	8

	Nos.
	
	

	6
	Collecting groundwater samples from boreholes for following chemical analysis after dewatering of boreholes.
a) pH
b) Sulphates in sample
c) Chlorides in sample
	4
	Nos.
	
	

	7
	Preservation soil and rock samples in wooden core boxes and forwarding selected soil, rock and water samples to laboratory for testing.
	1
	LS
	
	


BOQ FOR GEOTECHNICAL INVESTIGATION FOR 

PROPOSED ASPI BUILDING IN PASEO CLUSTER, SECTOR 3, PALAVA II
	SR

NO.
	DESCRIPTION OF ITEM
	ESTIMATED QUANTITY
	UNIT
	RATE
	AMOUNT (RS.)

	8
	Laboratory Testing on soil samples:

d) Grain Size Analysis

e) Hydrometer Analysis

f) Liquid Limit and Plastic Limit

g) pH, Sulphates, Chlorides in soil
	4
4
4
4
	Nos.
Nos.
Nos.
Nos.

	
	

	9
	Laboratory Testing on rock samples:

a) Dry Density

b) Water Absorption

c) Porosity 

d) Point Load Index Test

e) Unconfined Compressive Strength (UCS) Test
	4
4
4
4
4
	Nos.
Nos.
Nos.
Nos.
Nos.
	
	

	10
	Proving complete geotechnical report including results of all field and laboratory and detailed foundation recommendations, and addressing all relevant geotechnical issues.
	1 
	LS
	
	








TOTAL:








Taxes as Applicable:


GRAND TOTAL:

 

TOTAL IN WORDS:     









SEAL AND SIGNATURE OF CONTRACTOR:

