12.12.12
Palava–Space Nomenclature Definition
A: Built Blocks (includes mandatory open spaces but excludes built parking)
B: Built Parking (includes its mandatory open spaces)
C: Non-Built Blocks (includes open space > mandatory and includes the 10+5% structures permissible in open spaces)
Notes:
· A+B+C = 100% of gross plot
· All built forms, regardless of us, which are counted in FSI shall be part of A.
· Roads will mostly form part of A and B.
· Open Spaces will be significant portion of C and the non-road open space component of A, which are > 200 sm in contiguous size.
· Gross plot shall exclude following:
· Villages and Village extensions
· Guruchar or aakarpadit lands
· Lake
· Forest
· Any reservations which are ‘undesirable’ or ‘not needed in terms of our planning otherwise’ (though these reservations can be relocated within our land) eg. slaughterhouse, water storage facility
Naming of various areas in Phase 2
a. Sectors shall be numbered as 1…N. 
b. Clusters shall be numbered S.XXU (eg. 3.01L), where
a. S is the sector no.
b. XX is the two digit cluster no within a sector, starting from 01.
c. U is the nature of User, as follows:
i. O is office
ii. R is Retail
iii. E is EWS
iv. P is (predominantly) Public Space
v. A is Aspirational Residential
vi. L is Low Rise (upto 30 m) Casa
vii. M is Mid Rise (upto 70 m) Casa
viii. H is High rise (beyond 70 m) Casa
ix. V is (predominantly) Vehicular Parking
c. Wings shall be A…Z
