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To Mr. Ajay Saindansing
Project Lakeshore Greens (Sector 3)
Wing Elite (3.09A) — O wing (MODIFIED MIVAN)
Site Inspection Date 29/12/2014
Description
1. Peripheral
shuttering not
fixed.

2. Master Bedroom
& toilet area of
unit 1 & 2 were
already cast with
modified mivan.

1. The ground fioor
toilet windows of
unit 1 &2 were
cast as per tyj
floor windows.
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Switch boards on the non
structural walls were not
placed in the wall.
Instead some light points.
were seen (at different
heights) which are ot as
per dwg.

Beam reinforcement is not
placed properly in to the
column.

WIS inerts for the railing
not seen.
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| Sleeves yet to be fixed in
place

Lots of gaps seen in the
modified mivan formwork
which will lead to quality
issues.
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Congestion of conduits in
the slab & beam near DB
location, will lead to
Structural as well as
serious quality issues.

Levelling work in progress.
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LODHA GROUP

Soldier fixing of the Mivan
plates at the lift well still
pending

Balance points:

1. 45mm error found everywhere

2. Dowels to be left in the utility & the external chowk areas as
conveyed to Mr.venkatesh Kandikatti.

3. Al the ducts were in progress.

4. 200200 cut outs in the chajjas below the terraces were missing.

5. Fenestration dwg to be referred for all the wings for ground floor
openings.

6. Canopy was not yet cast.

Issued by :

b= sgnarures

Supriva Ambavane < Project Architect>





