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	Particulars
	Discussion
	Remarks

	Residential
	All the areas to be calculated on Net plot area.
Areas to be deducted from the gross plot are PG, Amenities, Schools.
Net Plot should have Mandatory RG, Building Footprint & Open Spaces.
	

	Residential
	Carpet Areas to be as per new optimized areas. They can be +/- 20sqft.
	

	
	Kitchen to have natural Ventilation.
	

	
	The bldg to be 5 to a core to be 4 nos 2 BHK’s & 1 no. 3 BHK. OR  Ideally
A  6 to a core with 4 nos  2 BHK’s & 2 no. 1 BHK.
	

	Residential
	[image: D:\D Drive\OFFICE DATA\PALAVA\PALAVA KHONI\CASA\ACTUAL\DRAWINGS\ARCHITECTURAL\MASTER PLAN\R14\FSI\G+17\54.9% G+17\ITP\MOM\NBC OPEN SPACES 2016.jpg]The open space rules will be as follows for bldgs up to 24m height:

Live to Live- H/3+H/3
Dead to dead- H/5+H/5
Live to dead - H/3+H/5

For bldgs above 24m height , the long length factor will be applicable plus the open space as per NBC.

Example:

For a cluster length of 100m & bldg height of 27m 
100-40=60m (Long length after every 40m)
10% of 60= 6m
Therefore 6m+9m (as per adjacent NBC table)= 15m
Hence the bldg to bldg clear distance will be 15m.
	

	Residential
	ROW to be 17m.
2m Footpath+ 4.5m parking+6m driveway+4.5m Parking.
	

	Residential
	The scissor staircase being longer & 1.5 m width (for both staircases) we should not be considering.
	

	Residential
	The elevators to be preferably side by side.
	

	
	The lobby ventilation can be through a full height window.
	

	
	The bldg height to be 3 m floor to floor.

	

	
	The bldg to be G+9
	

	
	The bldg to bldg distance to be 17m.
	

	
	The projection of the ‘T’ of the 6 to a core to be 6.5 m.
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