Points as discussed on 3rd March 2017
1. The reservations if completely owned can be shifted within 500m. If partly owned cannot be shifted.
2. Building to be at least 3m away from the RG.
3. Neighbourhood Center will comprise of the following:
a. 2 schools
b. PG for only required school.
c. Clubhouse
d. Temple
The area of the neighbourhood center will be about 28000sqm
4. EWS calculation as per Liaison are attached.
5. RG Options as per PBB plans.
a. Balance area to be developed is 519 acres.
b. RG requirement 7.5% & 5% = 12.5%
c. 10% is on Net Plot area. Therefore on Gross plot area will be 6.5%.
d. Therefore total of b & c will be 28% on Gross plot.
e. Hence RG requirement on 519 acres will be 145 acres i.e 399074 sm.

Option 1 (PBB)
RG as per pline is 331842sqm.
Deficit will be 67232 sqm.


Option 2 (PBB)
RG as per pline is 454610.76 sqm.
Surplus 61206  sqm.

Option 3 (PBB)
RG as per pline is 460280.917 sqm.
Surplus 55536  sqm.

6. Transport Hub cannot shift as it is not acquired 100%.
7. DP tweaking can be done but in acquired portion. The source of tweaking if not in the acquired area than the source cannot be tweaked.
8. ROW Sections
a. Main Spine 
Earlier it was 30.5m
Currently it is 42.5m as per Liaison. 
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b.  Internal road
6 + Refer table 4 of RP regulations  + 6
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9. Cycle Track
Liaison Team to take clarity on the physically segregated aspect of it.
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