











	Signage for, PALAVA 2 –SECTOR 3



1. FIRE HOSE REEL SIGNAGE

a. The symbol should be photo lumiscent.
b. Recommend using Prolite Autoglo stickers of size 150 x 150mm (6” x 6”) fixed on Sun board of same size.
c. [image: ]Please refer the image below for your working.










2. FIRE EXIT SIGNAGE

a. The text & thes ymbol should be photo lumiscent.
b. Recommend using Prolite Autoglo stickers of size 300 x 100mm (6” x 6”) fixed on Sun board of same size.
c. Please refer the image below for your working.
The board will be stuck on to the wall/door surface.	
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