
	SR.NO.
	INPUT PARAMETERS
	RESULTS
	LODHA POLICY
	Shaft Size in mm

	
	Typology
	NO.OF PASSENGERS 
	No. of Lifts
	SPEED m/sec
	WAITING INTERVAL sec
	5 MINUTES HANDLING CAPACITY
	WAITING INTERVAL sec
	5 MINUTES HANDLING CAPACITY
	Provided
(WxD)
	Proposed
(WxD)

	Project : Palava G+8
	 
	 
	 
	 

	1
	4 Apts per fl
	6
	1
	1.00
	81
	17.28%
	upto 75 sec
	5.00%
	2000x2000
	1800x1800

	2
	6 Apts per fl
	6
	1
	1.00
	81
	11.52%
	
	
	2000x2100
	1800x1800

	3
	
	8
	1
	1.00
	85
	14.78%
	
	
	2000x2100
	1800x1800

	Project : Palava G+20
	
	
	 
	 

	4
	2x2.5 BHK + 2x2 BHK
	10
	2
	1.50
	71
	11.71%
	
	
	2000x2581
	2100x2500

	5
	
	13
	2
	1.50
	74
	14.73%
	
	
	
	

	6
	2x1.5 BHK + 4x2 BHK
	13
	2
	1.50
	74
	11.05%
	
	
	2375x2500
	2100x2500



