6.9.13
Palava 2 – Residential Building Finishes


Gold
	Type
	Specification

	Air-conditioning
	Fully air-conditioned homes* with high quality split air-conditioner

	Flooring
	Living/dining & passage: Imported MabItal Flooring
Bedrooms: Classy imported Wooden flooring
Kitchen: High quality vitrified tiles
Toilets: High quality vitrified tiles

	CP & Sanitary Fittings
	High quality Jaquar CP fittings &European Duravit / Isenberg / Villeroy&Bochsanitaryware

	Floor to Floor Heights
	9’6” (for G+7); 10” (for G+19)

	Kitchen Finishes
	Granite Platform; stainless steel sink; piped gas connection**

	Key highlights of floor plan
	· Separate utility area in each apartment
· Separate store area in each apartment
· Separate wardrobe in each bedroom
· Deck in living / master bedroom or both
· Select apartments with lavish double height terraces

	Security
	World-class multi tier security with:
a. Automated Swipe card access to building
b. CCTV monitoring of entrance lobby and key public areas
c. Video doorphone

	Floor Lobby
	High quality vitrified tiles (2’ x 2’ or larger)

	Entrance Lobby
	Well decorated entrance lobby with imported MarbItal flooring

	Elevator
	Automatic elevators by Schindler /Otis/ ThyssenKrupp*
1 elevator as stretcher elevator in G+19 buildings

	Parking
	Open and covered options available

	Views
	Atleast 50% apartments with Garden views
All G+19 buildings with gardens/plaza on both sides

	Garden apartments
	Available with personal garden and kitchen yard

	Communication
	Provision for one telephone point in each apartment.
Advanced Fibre technology provision for high speed internet, digital gaming etc.

	Handicapped Access
	Special ramps for handicapped access to each entrance lobby





Platinum
	Type
	Specification

	Air-conditioning
	Fully air-conditioned homes* with high quality split air-conditioner

	Flooring
	Living/dining & passage: Italian marble flooring
Bedrooms: Classy imported Wooden flooring / Imported MarbItal Flooring
Kitchen: High quality vitrified tiles
Toilets: High quality vitrified tiles

	CP & Sanitary Fittings
	European Isenberg / High quality Jaquar CP fittings &European Duravit / Isenberg / Villeroy&Bochsanitaryware

	Floor to Floor Heights
	9’6” (for G+7); 10” (for G+19)

	Kitchen Finishes
	Fitted kitchen with international feel; double bowl stainless steel sink; piped gas connection**

	Key highlights of floor plan
	· Separate utility area in each apartment
· Separate store area in each apartment
· Separate wardrobe in each bedroom
· Deck in living / master bedroom or both
· Select apartments with lavish double height terraces

	Security
	World-class multi tier security with:
a. Automated Swipe card access to building
b. CCTV monitoring of entrance lobby and key public areas
c. Video doorphone

	Floor Lobby
	Imported MarbItal Flooring

	Entrance Lobby
	Designer entrance lobby with Italian Marble Flooring

	Elevator
	Automatic elevators by Schindler /Otis/ ThyssenKrupp*
1 elevator as stretcher elevator in G+19 buildings

	Parking
	Open and covered options available

	Views
	Atleast 50% apartments with Garden views
All G+19 buildings with gardens/plaza on both sides

	Garden apartments
	Available with personal garden and kitchen yard

	Communication
	Provision for one telephone point in each apartment.
Advanced Fibre technology provision for high speed internet, digital gaming etc.

	Handicapped Access
	Special ramps for handicapped access to each entrance lobby



Notes:
* Except kitchen, bathrooms and utility/service/servant areas
All brands stated above may be substituted with equivalent brands at the sole discretion of the project designer.
** Charges payable separately as stated in infrastructure charges; connection subject to approval and supply of gas from concerned authorities.
