22.05.13

SEAC meeting dated 22.05.13 
Compliances:
1. Examine soil capability of ponds for retaining water – 
Pond sections will be provided with impermeable clay liners to prevent seepage losses.
A typical sectional detail is awaited from PBB
2. 30m road connectivity to Dombivali – badalapur road – 
Refer attached dwg showing the connectivity as required.  
3. Street sweeping is a part of SWM plan.
Overall length of roads is 30kms. The cost is 45 paisa per month per sft of road.
 Hence Overall expenses will be about Rs.25.66 Crore annual for street maintenance.
4. Bio gas plant details – Awaiting from TCE.
5. STPs placed away from river – Awaiting from TCE.
6. Back up calculations for 2.2 lacs of tree plantation – Awaiting from PBB
7. CSR – 

8. Permissions / applications required as follows
(a) Commitment from nearby Fire brigade  to reun the proposed Fire station at Palava
(b) Letter from Grampanchayat  - crematorium
(c) Commitment from MMRDA for developing Sewer lines in the region.
(d) Multimodal corridor details from MMRDA
9. Toilet blocks for drivers in MLCPs. – Plan reqd.









