22.05.13

SEAC meeting dated 22.05.13 
Compliances:
1. Examine soil capability of ponds for retaining water – 
Pond sections will be provided with impermeable clay liners to prevent seepage losses.
A typical sectional detail is awaited from PBB
2. 30m road connectivity to Dombivali – badalapur road – 
Refer attached dwg showing the connectivity as required.  
3. Street sweeping is a part of SWM plan.
Overall length of roads is 30kms. The cost is 45 paisa per month per sft of road.
 Hence Overall expenses will be about -------- Crore annual for street maintenance.
4. Bio gas plant details – Awaiting from TCE.
5. STPs placed away from river – Awaiting from TCE.
6. Back up calculations for 2.2 lacs of tree plantation – Awaiting from PBB
7. CSR – 

8. Permissions / applications required as follows
(a) Commitment from nearby Fire brigade  to reun the proposed Fire station at Palava
(b) Letter from Grampanchayat  - crematorium
(c) Commitment from MMRDA for developing Sewer lines in the region.
(d) Multimodal corridor details from MMRDA
9. Toilet blocks for drivers in MLCPs. – Plan reqd.









